FSP Configuration
  Board "EK-RA4M2"
  R7FA4M2AD3CFP
    part_number: R7FA4M2AD3CFP
    rom_size_bytes: 524288
    ram_size_bytes: 131072
    data_flash_size_bytes: 8192
    package_style: LQFP
    package_pins: 100
    
  RA4M2
    series: 4
    
  RA4M2 Family
    Security: Exceptions: Exception Response: Non-Maskable Interrupt
    Security: Exceptions: BusFault, HardFault, and NMI Target: Secure State
    Security: System Reset Request Accessibility: Secure State
    Security: Exceptions: Prioritize Secure Exceptions: Disabled
    Security: Cache Accessibility: Both Secure and Non-Secure State
    Security: System Reset Status Accessibility: Both Secure and Non-Secure State
    Security: Battery Backup Accessibility: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM ECC: Both Secure and Non-Secure State
    Security: SRAM Accessibility: Standby RAM: Regions 7-0 are all Secure.
    Security: BUS Accessibility: Bus Security Attribution Register A: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register B: Both Secure and Non-Secure State
    Startup C-Cache Line Size: 32 Bytes
    OFS0 register settings: Independent WDT: Start Mode: IWDT is Disabled
    OFS0 register settings: Independent WDT: Timeout Period: 2048 cycles
    OFS0 register settings: Independent WDT: Dedicated Clock Frequency Divisor: 128
    OFS0 register settings: Independent WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: Independent WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: Independent WDT: Reset Interrupt Request Select: Reset is enabled
    OFS0 register settings: Independent WDT: Stop Control: Stop counting when in Sleep, Snooze mode, or Software Standby
    OFS0 register settings: WDT: Start Mode Select: Stop WDT after a reset (register-start mode)
    OFS0 register settings: WDT: Timeout Period: 16384 cycles
    OFS0 register settings: WDT: Clock Frequency Division Ratio: 128
    OFS0 register settings: WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: WDT: Reset Interrupt Request: Reset
    OFS0 register settings: WDT: Stop Control: Stop counting when entering Sleep mode
    OFS1 register settings: Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
    OFS1 register settings: Voltage Detection 0 Level: 2.80 V
    OFS1 register settings: HOCO Oscillation Enable: HOCO oscillation is disabled after reset
    Block Protection Settings (BPS): BPS0: 
    Permanent Block Protection Settings (PBPS): PBPS0: 
    Clocks: HOCO FLL Function: Disabled
    Main Oscillator Wait Time: 8163 cycles
    
  RA Common
    Main stack size (bytes): 0x400
    Heap size (bytes): 0x1000
    MCU Vcc (mV): 3300
    Parameter checking: Enabled
    Assert Failures: Return FSP_ERR_ASSERTION
    Error Log: No Error Log
    Clock Registers not Reset Values during Startup: Disabled
    Main Oscillator Populated: Populated
    PFS Protect: Enabled
    C Runtime Initialization : Enabled
    Early BSP Initialization : Disabled
    Main Oscillator Clock Source: Crystal or Resonator
    Subclock Populated: Populated
    Subclock Drive (Drive capacitance availability varies by MCU): Standard/Normal mode
    Subclock Stabilization Time (ms): 1000
    
  Clocks
    XTAL 24000000Hz
    HOCO 20MHz
    PLL Src: XTAL
    PLL Div /3
    PLL Mul x25.0
    PLL2 Disabled
    PLL2 Div /2
    PLL2 Mul x20.0
    Clock Src: PLL
    CLKOUT Disabled
    UCLK Disabled
    ICLK Div /2
    PCLKA Div /2
    PCLKB Div /4
    PCLKC Div /4
    PCLKD Div /2
    FCLK Div /4
    CLKOUT Div /1
    UCLK Div /5
    
  Pin Configurations
    RA4M2 EK -> g_bsp_pin_cfg
      AVCC0 88 ANALOG0_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 89 ANALOG0_AVSS0 - - - - - - - - IO "Read only" - 
      P000 100 ADC0_AN000 ARDUINO_A0_MIKROBUS_AN - - "Analog mode" - None "ADC0: AN000; ICU0: IRQ06" - IO - - 
      P001 99 ADC0_AN001 ARDUINO_A1 - - "Analog mode" - None "ADC0: AN001; ICU0: IRQ07" - IO - - 
      P002 98 ADC0_AN002 GROVE2_AN1 - - "Analog mode" - None "ADC0: AN002; ICU0: IRQ08" - IO - - 
      P003 97 ADC0_AN003 ARDUINO_A2 - - "Analog mode" - None "ADC0: AN003" - IO - - 
      P004 96 ADC0_AN004 GROVE2_AN2 - - "Analog mode" - None "ADC0: AN004; ICU0: IRQ09" - IO - - 
      P005 95 GPIO SW1 - IRQ10 "Input mode" - None "ADC0: AN005; ICU0: IRQ10" - IO - - 
      P006 94 GPIO SW2 - IRQ11 "Input mode" - None "ADC0: AN006; ICU0: IRQ11" - IO - - 
      P007 93 ADC0_AN007 ARDUINO_A3 - - "Analog mode" - None "ADC0: AN007" - IO - - 
      P008 92 GPIO PMOD1_INT - IRQ12 "Input mode" - "input pull-up" "ADC0: AN008; ICU0: IRQ12" - IO - - 
      P013 86 - - - - Disabled - - "ADC0: AN011; ANALOG0: VREFL" - None - - 
      P014 85 ADC0_AN012 ARDUINO_A4 - - "Analog mode" - None "ADC0: AN012; DAC0: DA0" - IO - - 
      P015 84 ADC0_AN013 ARDUINO_A5 - - "Analog mode" - None "ADC0: AN013; DAC1: DA1; ICU0: IRQ13" - IO - - 
      P100 75 SCI0_RXD0 ARDUINO_RX_MIKROBUS_RX Low None "Peripheral mode" CMOS None "AGT0: AGTIO0; GPT_POEG0: GTETRGA; GPT5: GTIOC5B; ICU0: IRQ02; QSPI0: QSPCLK; SCI0: RXD0; SCI0: SCL0; SCI1: SCK1" - IO - - 
      P101 74 SCI0_TXD0 ARDUINO_TX_MIKROBUS_TX Low None "Peripheral mode" CMOS None "AGT0: AGTEE0; GPT_POEG1: GTETRGB; GPT5: GTIOC5A; ICU0: IRQ01; QSPI0: QIO1; SCI0: SDA0; SCI0: TXD0; SCI1: CTSRTS1" - IO - - 
      P102 73 GPIO ARDUINO_D8 Low - "Output mode (Initial Low)" CMOS - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT_OPS0: GTOWLO; GPT2: GTIOC2B; QSPI0: QIO0; SCI0: SCK0" - IO - - 
      P103 72 GPIO ARDUINO_D6 Low - "Output mode (Initial Low)" CMOS - "AGT2: AGTIO2; CAN0: CTX0; GPT_OPS0: GTOWUP; GPT2: GTIOC2A; QSPI0: QIO3; SCI0: CTSRTS0" - IO - - 
      P104 71 QSPI0_QIO2 QSPI_IO2 Low None "Peripheral mode" CMOS None "AGT2: AGTEE2; GPT_POEG1: GTETRGB; GPT1: GTIOC1B; ICU0: IRQ01; QSPI0: QIO2" - IO - - 
      P105 70 GPIO ARDUINO_D3 Low None "Output mode (Initial Low)" CMOS - "AGT2: AGTO2; GPT_POEG0: GTETRGA; GPT1: GTIOC1A; ICU0: IRQ00" - IO - - 
      P106 69 GPIO ARDUINO_D4 Low - "Output mode (Initial Low)" CMOS - "AGT0: AGTOB0" - IO - - 
      P107 68 GPIO ARDUINO_D7 Low - "Output mode (Initial Low)" CMOS - "AGT0: AGTOA0" - IO - - 
      P108 51 DEBUG0_TMS - Low - "Peripheral mode" CMOS None "AGT3: AGTOA3; DEBUG0: SWDIO; DEBUG0: TMS; GPT_OPS0: GTOULO; GPT0: GTIOC0B; SCI9: CTSRTS9; SPI0: SSLA0" - IO - - 
      P109 52 DEBUG0_TDO - Low - "Peripheral mode" CMOS None "AGT3: AGTOB3; CGC0: CLKOUT; DEBUG0: TDO; DEBUG0: TRACESWO; GPT_OPS0: GTOVUP; GPT1: GTIOC1A; SCI9: SDA9; SCI9: TXD9; SPI0: MOSIA" - IO - - 
      P110 53 DEBUG0_TDI - Low None "Peripheral mode" CMOS None "AGT3: AGTEE3; DEBUG0: TDI; GPT_OPS0: GTOVLO; GPT1: GTIOC1B; ICU0: IRQ03; SCI2: CTSRTS2; SCI9: RXD9; SCI9: SCL9; SPI0: MISOA" - IO - - 
      P111 54 GPT3_GTIOC3A ARDUINO_D5_MIKROBUS_PWM Low None "Peripheral mode" CMOS None "AGT5: AGTOA5; GPT3: GTIOC3A; ICU0: IRQ04; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCKA" - IO - - 
      P112 55 SCI2_SDA2 ARDUINO_SDA_MIKROBUS_SDA Low - "Peripheral mode" "n-ch open drain" None "AGT5: AGTOB5; GPT3: GTIOC3B; QSPI0: QSSL; SCI1: SCK1; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA0; SSI0: SSIBCK0" - IO - - 
      P113 56 SCI2_SCL2 ARDUINO_SCL_MIKROBUS_SCL Low - "Peripheral mode" "n-ch open drain" None "AGT5: AGTEE5; GPT2: GTIOC2A; SCI2: RXD2; SCI2: SCL2; SSI0: SSILRCK0" - IO - - 
      P114 57 GPIO ARDUINO_D9 Low - "Output mode (Initial Low)" CMOS - "AGT5: AGTIO5; GPT2: GTIOC2B; SCI9: CTS9; SSI0: SSIRXD0" - IO - - 
      P115 58 GPIO ARDUINO_RST_MIKROBUS_RST Low - "Output mode (Initial Low)" CMOS - "GPT4: GTIOC4A; SSI0: SSITXD0" - IO - - 
      P200 40 - - - - Disabled - - "ICU0: NMI" - None - - 
      P201 39 - - - - Disabled - - "SYSTEM0: MD" - None - - 
      P205 32 - - - - Disabled - - "AGT1: AGTO1; CGC0: CLKOUT; CTSU0: TS01; GPT_OPS0: GTIV; GPT4: GTIOC4A; ICU0: IRQ01; IIC1: SCL1; SCI4: SDA4; SCI4: TXD4; SCI9: CTSRTS9; SDHI0: SD0DAT3; SPI0: SSLA0; SSI0: SSILRCK0; USB_FS0: USB_OVRCURA" - None - - 
      P206 31 SCI4_RXD4 PMOD1_MISO Low None "Peripheral mode" CMOS None "CTSU0: TS02; GPT_OPS0: GTIU; ICU0: IRQ00; IIC1: SDA1; SCI4: RXD4; SCI4: SCL4; SCI9: CTS9; SDHI0: SD0DAT2; SPI0: SSLA1; SSI0: SSIDATA0; USB_FS0: USB_VBUSEN" - IO - - 
      P207 30 SCI4_TXD4 PMOD1_MOSI Low - "Peripheral mode" CMOS None "CTSU0: TSCAP; QSPI0: QSSL; SCI4: SDA4; SCI4: TXD4; SPI0: SSLA2" - IO - - 
      P208 37 - - - - Disabled - - "GPT_OPS0: GTOVLO; QSPI0: QIO3; SDHI0: SD0DAT0" - None - - 
      P209 36 - - - - Disabled - - "AGT5: AGTEE5; GPT_OPS0: GTOVUP; QSPI0: QIO2; SDHI0: SD0WP" - None - - 
      P210 35 - - - - Disabled - - "AGT5: AGTOB5; GPT_OPS0: GTIW; QSPI0: QIO1; SDHI0: SD0CD" - None - - 
      P211 34 - - - - Disabled - - "AGT5: AGTOA5; GPT_OPS0: GTIV; QSPI0: QIO0; SDHI0: SD0CMD" - None - - 
      P212 14 CGC0_EXTAL - Low None "Peripheral mode" CMOS None "AGT1: AGTEE1; CGC0: EXTAL; GPT_POEG3: GTETRGD; GPT0: GTIOC0B; ICU0: IRQ03; SCI1: RXD1; SCI1: SCL1" - IO - - 
      P213 13 CGC0_XTAL - Low None "Peripheral mode" CMOS None "AGT2: AGTEE2; CGC0: XTAL; GPT_POEG2: GTETRGC; GPT0: GTIOC0A; ICU0: IRQ02; SCI1: SDA1; SCI1: TXD1" - IO - - 
      P214 33 - - - - Disabled - - "AGT5: AGTO5; GPT_OPS0: GTIU; QSPI0: QSPCLK; SDHI0: SD0CLK" - None - - 
      P300 50 DEBUG0_TCK - Low - "Peripheral mode" CMOS None "DEBUG0: SWCLK; DEBUG0: TCK; GPT_OPS0: GTOUUP; GPT0: GTIOC0A; SPI0: SSLA1" - IO - - 
      P301 49 - - - - Disabled - - "AGT0: AGTIO0; GPT_OPS0: GTOULO; GPT4: GTIOC4B; ICU0: IRQ06; SCI2: RXD2; SCI2: SCL2; SCI9: CTSRTS9; SPI0: SSLA2" - None - - 
      P302 48 - - - - Disabled - - "GPT_OPS0: GTOUUP; GPT4: GTIOC4A; ICU0: IRQ05; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA3" - None - - 
      P303 47 - - - - Disabled - - "GPT7: GTIOC7B; SCI9: CTS9" - None - - 
      P304 44 GPIO ARDUINO_D2 Low None "Output mode (Initial Low)" CMOS - "AGT2: AGTEE2; GPT_OPS0: GTOWLO; GPT7: GTIOC7A; ICU0: IRQ09" - IO - - 
      P305 43 QSPI0_QSPCLK QSPI_CLK Low None "Peripheral mode" CMOS None "AGT2: AGTOB2; GPT_OPS0: GTOWUP; ICU0: IRQ08; QSPI0: QSPCLK" - IO - - 
      P306 42 QSPI0_QSSL QSPI_CS Low - "Peripheral mode" CMOS None "AGT2: AGTOA2; GPT_OPS0: GTOULO; QSPI0: QSSL" - IO - - 
      P307 41 QSPI0_QIO0 QSPI_IO0 Low - "Peripheral mode" CMOS None "AGT4: AGTEE4; GPT_OPS0: GTOUUP; QSPI0: QIO0" - IO - - 
      P400 1 SCI4_SCK4 PMOD1_CLK Low None "Peripheral mode" CMOS None "AGT1: AGTIO1; GPT6: GTIOC6A; ICU0: IRQ00; IIC0: SCL0; SCI4: SCK4; SSI_COMMON0: AUDIO_CLK" - IO - - 
      P401 2 SCI4_CTSRTS4 PMOD1_SS Low None "Peripheral mode" CMOS None "CAN0: CTX0; GPT_POEG0: GTETRGA; GPT6: GTIOC6B; ICU0: IRQ05; IIC0: SDA0; SCI4: CTSRTS4" - IO - - 
      P402 3 GPIO PMOD1_IO1 Low None "Output mode (Initial Low)" CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC0: CACREF; CAN0: CRX0; ICU0: IRQ04; RTC0: RTCIC0; SCI4: CTS4; SSI_COMMON0: AUDIO_CLK" - IO - - 
      P403 4 GPIO PMOD1_RST Low None "Output mode (Initial Low)" CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; GPT3: GTIOC3A; ICU0: IRQ14; RTC0: RTCIC1; SSI0: SSIBCK0" - IO - - 
      P404 5 GPIO LED2 Low None "Output mode (Initial Low)" CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; GPT3: GTIOC3B; ICU0: IRQ15; RTC0: RTCIC2; SSI0: SSILRCK0" - IO - - 
      P405 6 GPIO LED3 Low - "Output mode (Initial Low)" CMOS - "GPT1: GTIOC1A; SSI0: SSITXD0" - IO - - 
      P406 7 GPIO PMOD1_IO2 Low - "Output mode (Initial Low)" CMOS - "AGT5: AGTO5; GPT1: GTIOC1B; SPI0: SSLA3; SSI0: SSIRXD0" - IO - - 
      P407 25 - - - - Disabled - - "ADC0: ADTRG0; AGT0: AGTIO0; CTSU0: TS03; GPT6: GTIOC6A; IIC0: SDA0; RTC0: RTCOUT; SCI4: CTSRTS4; SPI0: SSLA3; USB_FS0: USB_VBUS" - None - - 
      P408 24 SCI3_SCL3 GROVE1_SCL_QWIIC_SCL Low None "Peripheral mode" "n-ch open drain" None "AGT2: AGTOB2; CTSU0: TS04; GPT_OPS0: GTOWLO; GPT6: GTIOC6B; ICU0: IRQ07; IIC0: SCL0; SCI3: RXD3; SCI3: SCL3; SCI4: CTS4; USB_FS0: USB_ID" - IO - - 
      P409 23 SCI3_SDA3 GROVE1_SDA_QWIIC_SDA Low None "Peripheral mode" "n-ch open drain" None "AGT2: AGTOA2; CTSU0: TS05; GPT_OPS0: GTOWUP; ICU0: IRQ06; SCI3: SDA3; SCI3: TXD3; USB_FS0: USB_EXICEN" - IO - - 
      P410 22 - - - - Disabled - - "AGT1: AGTOB1; CTSU0: TS06; GPT_OPS0: GTOVLO; ICU0: IRQ05; SCI0: RXD0; SCI0: SCL0; SCI3: SCK3; SDHI0: SD0DAT1" - None - - 
      P411 21 - - - - Disabled - - "AGT1: AGTOA1; CTSU0: TS07; GPT_OPS0: GTOVUP; ICU0: IRQ04; SCI0: SDA0; SCI0: TXD0; SCI3: CTSRTS3; SDHI0: SD0DAT0" - None - - 
      P412 20 - - - - Disabled - - "AGT1: AGTEE1; CTSU0: TS08; GPT_OPS0: GTOULO; SCI0: SCK0; SCI3: CTS3; SDHI0: SD0CMD" - None - - 
      P413 19 SCI0_CTSRTS0 PMOD2_SS1 Low - "Peripheral mode" CMOS None "AGT3: AGTEE3; CTSU0: TS09; GPT_OPS0: GTOUUP; SCI0: CTSRTS0; SDHI0: SD0CLK" - IO - - 
      P414 18 GPIO PMOD2_INT - IRQ09 "Input mode" - "input pull-up" "AGT5: AGTIO5; CTSU0: TS10; GPT0: GTIOC0B; ICU0: IRQ09; SCI0: CTS0; SDHI0: SD0WP" - IO - - 
      P415 17 GPIO LED1 Low None "Output mode (Initial Low)" CMOS - "AGT4: AGTIO4; CTSU0: TS11; GPT0: GTIOC0A; ICU0: IRQ08; SDHI0: SD0CD; USB_FS0: USB_VBUSEN" - IO - - 
      P500 76 - - - - Disabled - - "ADC0: AN016; AGT0: AGTOA0; CAC0: CACREF; GPT_OPS0: GTIU; QSPI0: QSPCLK; USB_FS0: USB_VBUSEN" - None - - 
      P501 77 - - - - Disabled - - "AGT0: AGTOB0; GPT_OPS0: GTIV; ICU0: IRQ11; QSPI0: QSSL; USB_FS0: USB_OVRCURA" - None - - 
      P502 78 GPIO MIKROBUS_INT - IRQ12 "Input mode" - "input pull-up" "AGT2: AGTOA2; GPT_OPS0: GTIW; ICU0: IRQ12; QSPI0: QIO0; USB_FS0: USB_OVRCURB" - IO - - 
      P503 79 QSPI0_QIO1 QSPI_IO1 Low - "Peripheral mode" CMOS None "AGT2: AGTOB2; GPT_POEG2: GTETRGC; QSPI0: QIO1; USB_FS0: USB_EXICEN" - IO - - 
      P504 80 - - - - Disabled - - "AGT3: AGTOA3; GPT_POEG3: GTETRGD; QSPI0: QIO2; USB_FS0: USB_ID" - None - - 
      P505 81 QSPI0_QIO3 QSPI_IO3 Low None "Peripheral mode" CMOS None "AGT3: AGTOB3; ICU0: IRQ14; QSPI0: QIO3" - IO - - 
      P600 67 SCI9_SCK9 ARDUINO_CLK_MIKROBUS_CLK Low - "Peripheral mode" CMOS None "AGT3: AGTIO3; CAC0: CACREF; CGC0: CLKOUT; GPT6: GTIOC6B; SCI9: SCK9" - IO - - 
      P601 66 SCI9_RXD9 ARDUINO_MISO_MIKROBUS_MISO Low - "Peripheral mode" "n-ch open drain" None "AGT3: AGTEE3; GPT6: GTIOC6A; SCI9: RXD9; SCI9: SCL9" - IO - - 
      P602 65 SCI9_TXD9 ARDUINO_MOSI_MIKROBUS_MOSI Low - "Peripheral mode" "n-ch open drain" None "AGT3: AGTO3; GPT7: GTIOC7B; SCI9: SDA9; SCI9: TXD9" - IO - - 
      P603 64 SCI9_CTSRTS9 ARDUINO_SS_MIKROBUS_SS Low - "Peripheral mode" CMOS None "AGT4: AGTIO4; GPT7: GTIOC7A; SCI9: CTSRTS9" - IO - - 
      P608 59 GPIO PMOD2_RST Low - "Output mode (Initial Low)" CMOS - "GPT4: GTIOC4B" - IO - - 
      P609 60 GPIO PMOD2_IO1 Low - "Output mode (Initial Low)" CMOS - "AGT5: AGTO5; GPT5: GTIOC5A" - IO - - 
      P610 61 GPIO PMOD2_IO2 Low - "Output mode (Initial Low)" CMOS - "AGT4: AGTO4; GPT5: GTIOC5B" - IO - - 
      P708 16 - - - - Disabled - - "CAC0: CACREF; CTSU0: TS12; ICU0: IRQ11; SCI1: RXD1; SCI1: SCL1; SSI_COMMON0: AUDIO_CLK" - None - - 
      RES 38 SYSTEM0_RES - - - - - - - - IO "Read only" - 
      USBDM 27 USB_FS0_USB_DM - - - - - - - - IO "Read only" - 
      USBDP 28 USB_FS0_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 8 SYSTEM0_VBATT - - - - - - - - IO "Read only" - 
      VCC 15 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 46 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 62 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 82 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCCUSB 29 USB_FS0_VCC_USB - - - - - - - - IO "Read only" - 
      VCL0 9 SYSTEM0_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 87 ANALOG0_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 91 ANALOG0_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL0 90 ANALOG0_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 12 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 45 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 63 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 83 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSSUSB 26 USB_FS0_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 10 CGC0_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 11 CGC0_XCOUT - - - - - - - - IO "Read only" - 
    R7FA4M2AD3CFP.pincfg -> 
      AVCC0 88 ANALOG0_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 89 ANALOG0_AVSS0 - - - - - - - - IO "Read only" - 
      P000 100 - ARDUINO_A0_MIKROBUS_AN - - Disabled - None "ADC0: AN000; ICU0: IRQ06" - IO - - 
      P001 99 - ARDUINO_A1 - - Disabled - None "ADC0: AN001; ICU0: IRQ07" - IO - - 
      P002 98 - GROVE2_AN1 - - Disabled - None "ADC0: AN002; ICU0: IRQ08" - IO - - 
      P003 97 - ARDUINO_A2 - - Disabled - None "ADC0: AN003" - IO - - 
      P004 96 - GROVE2_AN2 - - Disabled - None "ADC0: AN004; ICU0: IRQ09" - IO - - 
      P005 95 - SW1 - None Disabled - None "ADC0: AN005; ICU0: IRQ10" - IO - - 
      P006 94 - SW2 - None Disabled - None "ADC0: AN006; ICU0: IRQ11" - IO - - 
      P007 93 - ARDUINO_A3 - - Disabled - None "ADC0: AN007" - IO - - 
      P008 92 - PMOD1_INT - None Disabled - None "ADC0: AN008; ICU0: IRQ12" - IO - - 
      P013 86 - - - - Disabled - - "ADC0: AN011; ANALOG0: VREFL" - None - - 
      P014 85 - ARDUINO_A4 - - Disabled - None "ADC0: AN012; DAC0: DA0" - IO - - 
      P015 84 - ARDUINO_A5 - - Disabled - None "ADC0: AN013; DAC1: DA1; ICU0: IRQ13" - IO - - 
      P100 75 - ARDUINO_RX_MIKROBUS_RX Low None Disabled CMOS None "AGT0: AGTIO0; GPT_POEG0: GTETRGA; GPT5: GTIOC5B; ICU0: IRQ02; QSPI0: QSPCLK; SCI0: RXD0; SCI0: SCL0; SCI1: SCK1" - IO - - 
      P101 74 - ARDUINO_TX_MIKROBUS_TX Low None Disabled CMOS None "AGT0: AGTEE0; GPT_POEG1: GTETRGB; GPT5: GTIOC5A; ICU0: IRQ01; QSPI0: QIO1; SCI0: SDA0; SCI0: TXD0; SCI1: CTSRTS1" - IO - - 
      P102 73 - ARDUINO_D8 Low - Disabled CMOS - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT_OPS0: GTOWLO; GPT2: GTIOC2B; QSPI0: QIO0; SCI0: SCK0" - IO - - 
      P103 72 - ARDUINO_D6 Low - Disabled CMOS - "AGT2: AGTIO2; CAN0: CTX0; GPT_OPS0: GTOWUP; GPT2: GTIOC2A; QSPI0: QIO3; SCI0: CTSRTS0" - IO - - 
      P104 71 - QSPI_IO2 Low None Disabled CMOS None "AGT2: AGTEE2; GPT_POEG1: GTETRGB; GPT1: GTIOC1B; ICU0: IRQ01; QSPI0: QIO2" - IO - - 
      P105 70 - ARDUINO_D3 Low None Disabled CMOS - "AGT2: AGTO2; GPT_POEG0: GTETRGA; GPT1: GTIOC1A; ICU0: IRQ00" - IO - - 
      P106 69 - ARDUINO_D4 Low - Disabled CMOS - "AGT0: AGTOB0" - IO - - 
      P107 68 - ARDUINO_D7 Low - Disabled CMOS - "AGT0: AGTOA0" - IO - - 
      P108 51 DEBUG0_TMS - Low - "Peripheral mode" CMOS None "AGT3: AGTOA3; DEBUG0: SWDIO; DEBUG0: TMS; GPT_OPS0: GTOULO; GPT0: GTIOC0B; SCI9: CTSRTS9; SPI0: SSLA0" - IO - - 
      P109 52 DEBUG0_TDO - Low - "Peripheral mode" CMOS None "AGT3: AGTOB3; CGC0: CLKOUT; DEBUG0: TDO; DEBUG0: TRACESWO; GPT_OPS0: GTOVUP; GPT1: GTIOC1A; SCI9: SDA9; SCI9: TXD9; SPI0: MOSIA" - IO - - 
      P110 53 DEBUG0_TDI - Low None "Peripheral mode" CMOS None "AGT3: AGTEE3; DEBUG0: TDI; GPT_OPS0: GTOVLO; GPT1: GTIOC1B; ICU0: IRQ03; SCI2: CTSRTS2; SCI9: RXD9; SCI9: SCL9; SPI0: MISOA" - IO - - 
      P111 54 - ARDUINO_D5_MIKROBUS_PWM Low None Disabled CMOS None "AGT5: AGTOA5; GPT3: GTIOC3A; ICU0: IRQ04; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCKA" - IO - - 
      P112 55 - ARDUINO_SDA_MIKROBUS_SDA Low - Disabled CMOS None "AGT5: AGTOB5; GPT3: GTIOC3B; QSPI0: QSSL; SCI1: SCK1; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA0; SSI0: SSIBCK0" - IO - - 
      P113 56 - ARDUINO_SCL_MIKROBUS_SCL Low - Disabled CMOS None "AGT5: AGTEE5; GPT2: GTIOC2A; SCI2: RXD2; SCI2: SCL2; SSI0: SSILRCK0" - IO - - 
      P114 57 - ARDUINO_D9 Low - Disabled CMOS - "AGT5: AGTIO5; GPT2: GTIOC2B; SCI9: CTS9; SSI0: SSIRXD0" - IO - - 
      P115 58 - ARDUINO_RST_MIKROBUS_RST Low - Disabled CMOS - "GPT4: GTIOC4A; SSI0: SSITXD0" - IO - - 
      P200 40 - - - - Disabled - - "ICU0: NMI" - None - - 
      P201 39 - - - - Disabled - - "SYSTEM0: MD" - None - - 
      P205 32 - - - - Disabled - - "AGT1: AGTO1; CGC0: CLKOUT; CTSU0: TS01; GPT_OPS0: GTIV; GPT4: GTIOC4A; ICU0: IRQ01; IIC1: SCL1; SCI4: SDA4; SCI4: TXD4; SCI9: CTSRTS9; SDHI0: SD0DAT3; SPI0: SSLA0; SSI0: SSILRCK0; USB_FS0: USB_OVRCURA" - None - - 
      P206 31 - PMOD1_MISO Low None Disabled CMOS None "CTSU0: TS02; GPT_OPS0: GTIU; ICU0: IRQ00; IIC1: SDA1; SCI4: RXD4; SCI4: SCL4; SCI9: CTS9; SDHI0: SD0DAT2; SPI0: SSLA1; SSI0: SSIDATA0; USB_FS0: USB_VBUSEN" - IO - - 
      P207 30 - PMOD1_MOSI Low - Disabled CMOS None "CTSU0: TSCAP; QSPI0: QSSL; SCI4: SDA4; SCI4: TXD4; SPI0: SSLA2" - IO - - 
      P208 37 - - - - Disabled - - "GPT_OPS0: GTOVLO; QSPI0: QIO3; SDHI0: SD0DAT0" - None - - 
      P209 36 - - - - Disabled - - "AGT5: AGTEE5; GPT_OPS0: GTOVUP; QSPI0: QIO2; SDHI0: SD0WP" - None - - 
      P210 35 - - - - Disabled - - "AGT5: AGTOB5; GPT_OPS0: GTIW; QSPI0: QIO1; SDHI0: SD0CD" - None - - 
      P211 34 - - - - Disabled - - "AGT5: AGTOA5; GPT_OPS0: GTIV; QSPI0: QIO0; SDHI0: SD0CMD" - None - - 
      P212 14 - - Low None Disabled CMOS None "AGT1: AGTEE1; CGC0: EXTAL; GPT_POEG3: GTETRGD; GPT0: GTIOC0B; ICU0: IRQ03; SCI1: RXD1; SCI1: SCL1" - IO - - 
      P213 13 - - Low None Disabled CMOS None "AGT2: AGTEE2; CGC0: XTAL; GPT_POEG2: GTETRGC; GPT0: GTIOC0A; ICU0: IRQ02; SCI1: SDA1; SCI1: TXD1" - IO - - 
      P214 33 - - - - Disabled - - "AGT5: AGTO5; GPT_OPS0: GTIU; QSPI0: QSPCLK; SDHI0: SD0CLK" - None - - 
      P300 50 DEBUG0_TCK - Low - "Peripheral mode" CMOS None "DEBUG0: SWCLK; DEBUG0: TCK; GPT_OPS0: GTOUUP; GPT0: GTIOC0A; SPI0: SSLA1" - IO - - 
      P301 49 - - - - Disabled - - "AGT0: AGTIO0; GPT_OPS0: GTOULO; GPT4: GTIOC4B; ICU0: IRQ06; SCI2: RXD2; SCI2: SCL2; SCI9: CTSRTS9; SPI0: SSLA2" - None - - 
      P302 48 - - - - Disabled - - "GPT_OPS0: GTOUUP; GPT4: GTIOC4A; ICU0: IRQ05; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA3" - None - - 
      P303 47 - - - - Disabled - - "GPT7: GTIOC7B; SCI9: CTS9" - None - - 
      P304 44 - ARDUINO_D2 Low None Disabled CMOS - "AGT2: AGTEE2; GPT_OPS0: GTOWLO; GPT7: GTIOC7A; ICU0: IRQ09" - IO - - 
      P305 43 - QSPI_CLK Low None Disabled CMOS None "AGT2: AGTOB2; GPT_OPS0: GTOWUP; ICU0: IRQ08; QSPI0: QSPCLK" - IO - - 
      P306 42 - QSPI_CS Low - Disabled CMOS None "AGT2: AGTOA2; GPT_OPS0: GTOULO; QSPI0: QSSL" - IO - - 
      P307 41 - QSPI_IO0 Low - Disabled CMOS None "AGT4: AGTEE4; GPT_OPS0: GTOUUP; QSPI0: QIO0" - IO - - 
      P400 1 - PMOD1_CLK Low None Disabled CMOS None "AGT1: AGTIO1; GPT6: GTIOC6A; ICU0: IRQ00; IIC0: SCL0; SCI4: SCK4; SSI_COMMON0: AUDIO_CLK" - IO - - 
      P401 2 - PMOD1_SS Low None Disabled CMOS None "CAN0: CTX0; GPT_POEG0: GTETRGA; GPT6: GTIOC6B; ICU0: IRQ05; IIC0: SDA0; SCI4: CTSRTS4" - IO - - 
      P402 3 - PMOD1_IO1 Low None Disabled CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC0: CACREF; CAN0: CRX0; ICU0: IRQ04; RTC0: RTCIC0; SCI4: CTS4; SSI_COMMON0: AUDIO_CLK" - IO - - 
      P403 4 - PMOD1_RST Low None Disabled CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; GPT3: GTIOC3A; ICU0: IRQ14; RTC0: RTCIC1; SSI0: SSIBCK0" - IO - - 
      P404 5 - LED2 Low None Disabled CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; GPT3: GTIOC3B; ICU0: IRQ15; RTC0: RTCIC2; SSI0: SSILRCK0" - IO - - 
      P405 6 - LED3 Low - Disabled CMOS - "GPT1: GTIOC1A; SSI0: SSITXD0" - IO - - 
      P406 7 - PMOD1_IO2 Low - Disabled CMOS - "AGT5: AGTO5; GPT1: GTIOC1B; SPI0: SSLA3; SSI0: SSIRXD0" - IO - - 
      P407 25 - - - - Disabled - - "ADC0: ADTRG0; AGT0: AGTIO0; CTSU0: TS03; GPT6: GTIOC6A; IIC0: SDA0; RTC0: RTCOUT; SCI4: CTSRTS4; SPI0: SSLA3; USB_FS0: USB_VBUS" - None - - 
      P408 24 - GROVE1_SCL_QWIIC_SCL Low None Disabled CMOS None "AGT2: AGTOB2; CTSU0: TS04; GPT_OPS0: GTOWLO; GPT6: GTIOC6B; ICU0: IRQ07; IIC0: SCL0; SCI3: RXD3; SCI3: SCL3; SCI4: CTS4; USB_FS0: USB_ID" - IO - - 
      P409 23 - GROVE1_SDA_QWIIC_SDA Low None Disabled CMOS None "AGT2: AGTOA2; CTSU0: TS05; GPT_OPS0: GTOWUP; ICU0: IRQ06; SCI3: SDA3; SCI3: TXD3; USB_FS0: USB_EXICEN" - IO - - 
      P410 22 - - - - Disabled - - "AGT1: AGTOB1; CTSU0: TS06; GPT_OPS0: GTOVLO; ICU0: IRQ05; SCI0: RXD0; SCI0: SCL0; SCI3: SCK3; SDHI0: SD0DAT1" - None - - 
      P411 21 - - - - Disabled - - "AGT1: AGTOA1; CTSU0: TS07; GPT_OPS0: GTOVUP; ICU0: IRQ04; SCI0: SDA0; SCI0: TXD0; SCI3: CTSRTS3; SDHI0: SD0DAT0" - None - - 
      P412 20 - - - - Disabled - - "AGT1: AGTEE1; CTSU0: TS08; GPT_OPS0: GTOULO; SCI0: SCK0; SCI3: CTS3; SDHI0: SD0CMD" - None - - 
      P413 19 - PMOD2_SS1 Low - Disabled CMOS None "AGT3: AGTEE3; CTSU0: TS09; GPT_OPS0: GTOUUP; SCI0: CTSRTS0; SDHI0: SD0CLK" - IO - - 
      P414 18 - PMOD2_INT - None Disabled - None "AGT5: AGTIO5; CTSU0: TS10; GPT0: GTIOC0B; ICU0: IRQ09; SCI0: CTS0; SDHI0: SD0WP" - IO - - 
      P415 17 - LED1 Low None Disabled CMOS - "AGT4: AGTIO4; CTSU0: TS11; GPT0: GTIOC0A; ICU0: IRQ08; SDHI0: SD0CD; USB_FS0: USB_VBUSEN" - IO - - 
      P500 76 - - - - Disabled - - "ADC0: AN016; AGT0: AGTOA0; CAC0: CACREF; GPT_OPS0: GTIU; QSPI0: QSPCLK; USB_FS0: USB_VBUSEN" - None - - 
      P501 77 - - - - Disabled - - "AGT0: AGTOB0; GPT_OPS0: GTIV; ICU0: IRQ11; QSPI0: QSSL; USB_FS0: USB_OVRCURA" - None - - 
      P502 78 - MIKROBUS_INT - None Disabled - None "AGT2: AGTOA2; GPT_OPS0: GTIW; ICU0: IRQ12; QSPI0: QIO0; USB_FS0: USB_OVRCURB" - IO - - 
      P503 79 - QSPI_IO1 Low - Disabled CMOS None "AGT2: AGTOB2; GPT_POEG2: GTETRGC; QSPI0: QIO1; USB_FS0: USB_EXICEN" - IO - - 
      P504 80 - - - - Disabled - - "AGT3: AGTOA3; GPT_POEG3: GTETRGD; QSPI0: QIO2; USB_FS0: USB_ID" - None - - 
      P505 81 - QSPI_IO3 Low None Disabled CMOS None "AGT3: AGTOB3; ICU0: IRQ14; QSPI0: QIO3" - IO - - 
      P600 67 - ARDUINO_CLK_MIKROBUS_CLK Low - Disabled CMOS None "AGT3: AGTIO3; CAC0: CACREF; CGC0: CLKOUT; GPT6: GTIOC6B; SCI9: SCK9" - IO - - 
      P601 66 - ARDUINO_MISO_MIKROBUS_MISO Low - Disabled CMOS None "AGT3: AGTEE3; GPT6: GTIOC6A; SCI9: RXD9; SCI9: SCL9" - IO - - 
      P602 65 - ARDUINO_MOSI_MIKROBUS_MOSI Low - Disabled CMOS None "AGT3: AGTO3; GPT7: GTIOC7B; SCI9: SDA9; SCI9: TXD9" - IO - - 
      P603 64 - ARDUINO_SS_MIKROBUS_SS Low - Disabled CMOS None "AGT4: AGTIO4; GPT7: GTIOC7A; SCI9: CTSRTS9" - IO - - 
      P608 59 - PMOD2_RST Low - Disabled CMOS - "GPT4: GTIOC4B" - IO - - 
      P609 60 - PMOD2_IO1 Low - Disabled CMOS - "AGT5: AGTO5; GPT5: GTIOC5A" - IO - - 
      P610 61 - PMOD2_IO2 Low - Disabled CMOS - "AGT4: AGTO4; GPT5: GTIOC5B" - IO - - 
      P708 16 - - - - Disabled - - "CAC0: CACREF; CTSU0: TS12; ICU0: IRQ11; SCI1: RXD1; SCI1: SCL1; SSI_COMMON0: AUDIO_CLK" - None - - 
      RES 38 SYSTEM0_RES - - - - - - - - IO "Read only" - 
      USBDM 27 USB_FS0_USB_DM - - - - - - - - IO "Read only" - 
      USBDP 28 USB_FS0_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 8 SYSTEM0_VBATT - - - - - - - - IO "Read only" - 
      VCC 15 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 46 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 62 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 82 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCCUSB 29 USB_FS0_VCC_USB - - - - - - - - IO "Read only" - 
      VCL0 9 SYSTEM0_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 87 ANALOG0_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 91 ANALOG0_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL0 90 ANALOG0_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 12 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 45 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 63 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 83 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSSUSB 26 USB_FS0_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 10 CGC0_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 11 CGC0_XCOUT - - - - - - - - IO "Read only" - 
    
  User Events
    
  User Event Links
    
  Module "I/O Port (r_ioport)"
    Parameter Checking: Default (BSP)
    
  Module "Azure RTOS ThreadX Port (rm_threadx_port)"
  Module "Azure RTOS NetX Duo IP Instance"
    Common: Error Checking: Enabled (default)
    Common: IP Packet Filter: Disabled (default)
    Common: IP Static Routing: Disabled (default)
    Common: Physical Header: 
    Common: Physical Trailer: 
    Common: ARP Defend By Reply: Disabled (default)
    Common: ARP Mac Change Notification: Disabled (default)
    Common: ARP Expiration Rate: 
    Common: ARP Update Rate: 
    Common: TCP ACK Timer Rate: 
    Common: TCP Fast Timer Rate: 
    Common: TCP Transmit Timer Rate: 
    Common: TCP Keepalive Initial: 
    Common: TCP Keepalive Retry Interval: 
    Common: ARP Maximum Retries: 
    Common: ARP Maximum Queue Depth: 
    Common: ARP Auto ARP Entry: Enabled (default)
    Common: Maximum Multicast Groups: 
    Common: Maximum Listen Requests: 
    Common: TCP Keepalive: Disabled (default)
    Common: TCP Window Scaling: Disabled (default)
    Common: TCP Immediate ACK: Disabled (default)
    Common: TCP ACK Every N Packets: 
    Common: TCP Maximum Retries: 
    Common: TCP Maximum TX Queue: 
    Common: TCP Retry Shift: 
    Common: TCP Keepalive Retries: 
    Common: Driver Deferred Processing: Disabled (default)
    Common: Loopback Interface: Enabled (default)
    Common: Maximum Physical Interfaces: 
    Common: Fragmentation support: Enabled (default)
    Common: IP RX Checksum: Enabled (default)
    Common: IP TX Checksum: Enabled (default)
    Common: TCP RX Checksum: Enabled (default)
    Common: TCP TX Checksum: Enabled (default)
    Common: UDP RX Checksum: Enabled (default)
    Common: UDP TX Checksum: Enabled (default)
    Common: Reset Disconnect: Enabled (default)
    Common: RX Size Checking: Enabled (default)
    Common: ARP Info: Enabled (default)
    Common: IP Info: Enabled (default)
    Common: ICMP Info: Enabled (default)
    Common: IGMPv2: Enabled (default)
    Common: IGMP Info: Enabled (default)
    Common: Packet Info: Enabled (default)
    Common: RARP Info: Enabled (default)
    Common: TCP Info: Enabled (default)
    Common: UDP Info: Enabled (default)
    Common: Extended Notify Support: Disabled (default)
    Common: NAT: Disabled (default)
    Common: Packet Header Pad Size: 
    Common: TCP MSS Minimum: 
    Common: Source Address Check: Disabled (default)
    Common: ARP Defend Interval: 
    Common: TCP Maximum Out Of Order Packets: 
    Common: NetX Duo IPV6 Support: Disabled
    Common: Notify when the IPv6 address is changed: Disabled (default)
    Common: Allow discover maximum MTU in the path: Disabled (default)
    Common: Wait before resetting target's path MTU in destination table (seconds): 
    Common: IPv6 routing table entry limit: 
    Common: IPv6 destination table entry limit: 
    Common: Maximum time allowed to reassemble IP fragment: 
    Common: Maximum time allowed to reassemble IPv4 fragment: 
    Common: Maximum time allowed to reassemble IPv6 fragment: 
    Common: IPv6 multicast join/leave function support: Disabled (default)
    Common: Size of the prefix table for router advertisements: 
    Common: Stateless address auto-configuration support: Disabled (default)
    Common: IPv6 address pool entry limit: 
    Common: Delay before the first stale cache entry solicitation (seconds): 
    Common: Duplicate Address Detection support: Enabled (default)
    Common: Neighbor Solicitation message count before interface address marked valid: 
    Common: Retain older cache table entries till timeout option: Disabled (default)
    Common: IPv6 Neighbor Cache table entry limit.: 
    Common: Neighbor Solicitation message count for IPv6 Neighbor Discovery protocol: 
    Common: Neighbor Solicitation message count to determine neighbor’s reachability: 
    Common: Maximum entries in ND cache queue: 
    Common: Duration for address to be 'reachable' with no packets received from it (seconds): 
    Common: Delay between solicitation packets (milliseconds): 
    Common: ICMPv6 error message in response to invalid packet support: Enabled (default)
    Common: ICMPv6 redirect packet processing support: Enabled (default)
    Common: IPv6 router advertisement packet processing support: Enabled (default)
    Common: Periodic IPv6 router solicitation messages support: Enabled (default)
    Common: Maximum host router solicitations till no response is received: 
    Common: Interval between two router solicitation messages: 
    Common: Checksum computation support on received ICMPv4 packets: Enabled (default)
    Common: Checksum computation support on received ICMPv6 packets: Enabled (default)
    Common: Checksum computation support on received ICMP packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMPv4 packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMPv6 packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMP packets: Enabled (default)
    Common: Packet Alignment: 
    Common: Random Number Generator: rand
    Common: Seed Random Number Generator: srand
    DHCP: Common: IPv4: Type of Service for UDP requests: Normal
    DHCP: Common: IPv4: Fragmentation option: Don't fragment
    DHCP: Common: IPv4: Time to live: 128
    DHCP: Common: IPv4: Packet Queue depth: 5
    DHCP: Client: IPv4: Internal thread priority: 3
    DHCP: Client: IPv4: Internal thread stack size (bytes): 4096
    DHCP: Client: IPv4: Timeout between DHCP messages processed (seconds): 1
    DHCP: Client: IPv4: Use BOOTP: Disable
    DHCP: Client: IPv4: Send ARP probe: Disable
    DHCP: Client: IPv4: ARP probe wait time (seconds): 1
    DHCP: Client: IPv4: Minimum ARP probe wait time (seconds): 1
    DHCP: Client: IPv4: Maximum ARP probe wait time (seconds): 2
    DHCP: Client: IPv4: ARP probe count: 2
    DHCP: Client: IPv4: Maximum retransmission timeout (seconds): 64
    DHCP: Client: IPv4: Minimum renew timeout (seconds): 60
    DHCP: Client: IPv4: Minimum retransmission timeout (seconds): 4
    DHCP: Client: IPv4: Persistent client state: Disable
    DHCP: Client: IPv4: Maximum message size support: Disable
    DHCP: Client: IPv4: DHCP options buffer size (bytes): 312
    DHCP: Client: IPv4: Maximum number of network interfaces for DHCP client: 1
    DHCP: Client: IPv4: Wait before restarting the configuration process (seconds): 10
    HTTP: Common: Type of Service: Normal
    HTTP: Common: Fragmentation option: Don't fragment
    HTTP: Common: Time to live: 128
    HTTP: Common: MD5 Support: Disable
    HTTP: Common: Maximum resource name length (bytes): 40
    HTTP: Common: Maximum password length (bytes): 20
    HTTP: Common: Maximum username length (bytes): 20
    HTTP: Client: Minimum packet size (bytes): 600
    HTTP: Client: Operation timeout (seconds): 10
    DNS: Client: DNS Control Type of Service: Normal
    DNS: Client: Socket fragmentation option: Dont fragment
    DNS: Client: Time to live: 128
    DNS: Client: Client DNS IP version: IPv4
    DNS: Client: Maximum number of DNS Servers in the Client server list: 5
    DNS: Client: Maximum DNS queries size (bytes): 512
    DNS: Client: Maximum retries for a server: 3
    DNS: Client: Maximum duration to retransmit a DNS query (seconds): 64
    DNS: Client: Packet allocate timeout (seconds): 1
    DNS: Client: Client has DNS and Gateway server: Disable
    DNS: Client: Clear previous DNS queries from queue: Disable
    DNS: Client: Extended RR types support: Disable
    DNS: Client: Cache support: Disable
    Telnet: Common: Type of service for TCP requests: Normal
    Telnet: Common: Fragmentation option: Don't fragment
    Telnet: Common: Server TCP port number: 23
    Telnet: Common: Time to live: 128
    AutoIP: Wait before sending first probe (seconds): 1
    AutoIP: ARP probes to send: 3
    AutoIP: Minimum wait between probes (seconds): 1
    AutoIP: Maximum wait between probes (seconds): 2
    AutoIP: Maximum conflicts before increasing processing delay: 10
    AutoIP: Wait extend after maximum conflicts (seconds): 60
    AutoIP: Wait before announcement (seconds): 2
    AutoIP: Number of ARP announces: 2
    AutoIP: Wait between announces (seconds): 2
    AutoIP: Wait between defense announces (seconds): 10
    Web HTTP: Common: Type of Service: Normal
    Web HTTP: Common: Fragmentation option: Don't fragment
    Web HTTP: Common: MD5 Support: Disable
    Web HTTP: Common: Time to live: 128
    Web HTTP: Common: Maximum password length (bytes): 20
    Web HTTP: Common: Maximum username length (bytes): 20
    Web HTTP: Client: Minimum packet size (bytes): 300
    Web HTTP: Client: HTTPS Support: Disable
    SMTP: Client: TCP window size (bytes): 1460
    SMTP: Client: Packet allocation timeout (seconds): 2
    SMTP: Client: TCP socket connect timeout (seconds): 10
    SMTP: Client: TCP socket disconnect timeout (seconds): 5
    SMTP: Client: Server greeting reply timeout (seconds): 10
    SMTP: Client: Command timeout (seconds): 10
    SMTP: Client: Mail data request timeout (seconds): 30
    SMTP: Client: TCP socket send completion timeout (seconds): 5
    SMTP: Client: Server challenge maximum string length (bytes): 200
    SMTP: Client: Maximum password length (bytes): 20
    SMTP: Client: Maximum username length (bytes): 40
    DHCP: Client: IPv6: Internal thread priority: 3
    DHCP: Client: IPv6: Time out for obtaining DHCPv6 client mutex (ticks): TX_WAIT_FOREVER
    DHCP: Client: IPv6: Time interval between current IP address lease time update (seconds): 1
    DHCP: Client: IPv6: Maximum IA addresses allowed in client record: 1
    DHCP: Client: IPv6: Number of DNS servers the client will store: 2
    DHCP: Client: IPv6: Number of time servers the client will store: 1
    DHCP: Client: IPv6: Domain name buffer size (bytes): 32
    DHCP: Client: IPv6: Current time zone information buffer size (bytes): 16
    DHCP: Client: IPv6: Maximum DHCPv6 server messages buffer size (bytes): 100
    DHCP: Common: IPv6: Type of Service for UDP requests: Normal
    DHCP: Common: IPv6: Time to live: 128
    DHCP: Common: IPv6: Packet Queue depth: 5
    DHCP: Common: IPv6: Packet allocation timeout (seconds): 3
    DHCP: Common: IPv6: Interval for active session time update (seconds): 3
    DHCP: Server: IPv4: Internal thread priority: 2
    DHCP: Server: IPv4: Packet allocate timeout (seconds): 2
    DHCP: Server: IPv4: Fast periodic timer interval to check session inactivity timeout (seconds): 10
    DHCP: Server: IPv4: DHCP Client Session timeout - multiple of Fast periodic interval (seconds): 10
    DHCP: Server: IPv4: Client IP address default lease time (seconds): 0xFFFFFFFF
    DHCP: Server: IPv4: Slow periodic timer interval to check IP lease expiration (seconds): 1000
    DHCP: Server: IPv4: Size of the array to contain options in client request (units): 12
    DHCP: Server: IPv4: Server option list (optional - use space for separation) : 1 3 6
    DHCP: Server: IPv4: Server option list size (optional): 3
    DHCP: Server: IPv4: Size of the server host name buffer (bytes): 32
    DHCP: Server: IPv4: Size of the current client hostname buffer (bytes): 32
    DHCP: Server: IPv4: Maximum size of an IP addresses list (units): 20
    DHCP: Server: IPv4: Size of client record table (units): 50
    DHCP: Server: IPv4: Size of the BOOT buffer (bytes): 548
    DHCP: Server: IPv6: Internal thread priority: 2
    DHCP: Server: IPv6: Client lease time expiration check interval (seconds): 60
    DHCP: Server: IPv6: DHCPv6 packet receive timeout (seconds): 1
    DHCP: Server: IPv6: Server preference ranking for clients: 0
    DHCP: Server: IPv6: Maximum options to extract from a client message: 6
    DHCP: Server: IPv6: Server interval for first client IP address renewal attempt (seconds): 2000
    DHCP: Server: IPv6: Server interval for second client IP address renewal attempt (seconds): 3000
    DHCP: Server: IPv6: Time interval after which client IP is deprecated (seconds): 2 * NX_DHCPV6_DEFAULT_T1_TIME
    DHCP: Server: IPv6: Time interval after which leased IP is invalid (seconds): 2 * NX_DHCPV6_DEFAULT_PREFERRED_TIME
    DHCP: Server: IPv6: Maximum server status option message size (bytes): 100
    DHCP: Server: IPv6: Maximum Size of the Server’s IP lease table (count): 100
    DHCP: Server: IPv6: Size of the Server’s Client record table (count): 120
    DHCP: Server: IPv6: Server socket fragmentation option: Dont fragment
    DHCP: Server: IPv6: Vendor assigned unique ID: abcdeffghijklmnopqrstuvwxyz
    DHCP: Server: IPv6: Private vendor ID: 0x12345678
    DHCP: Server: IPv6: Size of Vendor ID buffer (bytes): 48
    DHCP: Server: IPv6: Client request success message : granted: IA OPTION GRANTED
    DHCP: Server: IPv6: Client request failure message : Failure unspecified: IA OPTION NOT GRANTED-FAILURE UNSPECIFIED
    DHCP: Server: IPv6: Client request failure message : No addresses available: IA OPTION NOT GRANTED-NO ADDRESSES AVAILABLE
    DHCP: Server: IPv6: Client request failure message : Invalid client request: IA OPTION NOT GRANTED-INVALID CLIENT REQUEST
    DHCP: Server: IPv6: Client request failure message : Client not on link: IA OPTION NOT GRANTED-CLIENT NOT ON LINK
    DHCP: Server: IPv6: Client request failure message : Client must use multicast: IA OPTION NOT GRANTED-CLIENT MUST USE MULTICAST
    DHCP: Server: IPv6: Session inactivity timeout(seconds): 20
    Telnet: Server: Internal thread priority: 16
    Telnet: Server: Maximum clients to serve simultaneously: 4
    Telnet: Server: Socket window size (bytes): 2048
    Telnet: Server: Server time out (seconds): 10
    Telnet: Server: Client inactivity timeout (seconds): 600
    Telnet: Server: Timeout check period (seconds): 60
    Telnet: Server: Option negotiation: Enable
    Telnet: Server: Use application packet pool: Disable
    Telnet: Server: Packet size in the pool (bytes): 300
    Telnet: Server: Total packet pool size (bytes): 2048
    SNTP: Client: Internal thread stack size (bytes): 2048
    SNTP: Client: SNTP client thread time slicing interval (ticks): TX_NO_TIME_SLICE
    SNTP: Client: Internal thread priority: 2
    SNTP: Client: UDP socket name: SNTP Client socket
    SNTP: Client: UDP port number: 123
    SNTP: Client: Server UDP port: 123
    SNTP: Client: Time to live: 128
    SNTP: Client: Maximum UDP packets queue depth (units): 5
    SNTP: Client: Packet allocation timeout (seconds): 1
    SNTP: Client: SNTP version to use: 3
    SNTP: Client: NTP minimum version: 3
    SNTP: Client: Lowest level server stratum client accepts: 2
    SNTP: Client: Minimum time difference that triggers adjustment (milliseconds): 10
    SNTP: Client: Maximum time adjustment allowed to local clock time (milliseconds): 180000
    SNTP: Client: Ignore maximum time adjust limit at startup: True
    SNTP: Client: Maximum time lapse without valid update (seconds): 7200
    SNTP: Client: 'Update time remaining' timer update interval (seconds): 1
    SNTP: Client: Starting poll interval for unicast update request (seconds): 3600
    SNTP: Client: Poll interval increment after failed time update: 2
    SNTP: Client: Calculate round trip time of messages: False
    SNTP: Client: Maximum server clock inaccuracy to accept (to disable set 0): 50000
    SNTP: Client: Invalid message limit to mark server invalid: 3
    SNTP: Client: Randomize update request interval on startup: False
    SNTP: Client: Internal Task sleep interval (ticks): 1
    SNTP: Client: Current calendar year: 2016
    TFTP: Common: Maximum error string length (bytes): 64
    TFTP: Common: Time to live: 128
    TFTP: Common: Type of Service for UDP requests: Normal
    TFTP: Common: Fragmentation option: Don't fragment
    TFTP: Client: Source port to use: NX_ANY_PORT
    MQTT: Client: NX Secure: Disable
    MQTT: Client: Cloud Enable: Disable
    MQTT: Client: Keepalive Timer Rate (s): 1
    MQTT: Client: Ping Timeout Delay (s): 1
    MQTT: Client: Socket Timeout (in timer ticks) : 0xFFFFFFFF
    NAT: Minimum count for translation entry: 3
    NAT: Timeout for translation entry (seconds): 240
    NAT: Minimum assigned port number for outbound TCP packets: 20000
    NAT: Maximum assigned port number for outbound TCP packets: 30000
    NAT: Minimum assigned port number for outbound UDP packets: 20000
    NAT: Maximum assigned port number for outbound UDP packets: 30000
    NAT: Minimum ICMP query identifier: 20000
    NAT: Maximum ICMP query identifier: 30000
    FTP: Common: Control Type of Service: Normal
    FTP: Common: Data Type of Service: Normal
    FTP: Common: Fragmentation option: Don't fragment
    FTP: Common: Time to live: 128
    FTP: Common: Duration between client inactivity check (seconds): 60
    FTP: Client: TCP socket to use: NX_ANY_PORT
    SNMP: Agent: Internal thread stack size (bytes): 4096
    SNMP: Agent: SNMP agent priority: 16
    SNMP: Agent: Type of service for SNMP responses: Normal
    SNMP: Agent: Fragment enable for SNMP PDU requests: Dont Fragment
    SNMP: Agent: SNMP socket time to live: 128
    SNMP: Agent: Agent timeout: 100
    SNMP: Agent: Max octet string size: 255
    SNMP: Agent: Max context string size: 32
    SNMP: Agent: Max User name Size: 64
    SNMP: Agent: Max security Key Size: 64
    SNMP: Agent: Maximum SNMP packet size: 560
    SNMP: Agent: UDP port number: 161
    SNMP: Agent: Trap destination port: 162
    SNMP: Agent: Max trap Key Size: 64
    SNMP: Agent: SNMP Version 1: Enable
    SNMP: Agent: SNMP Version 2: Enable
    SNMP: Agent: SNMP Version 3: Enable
    POP3: Client: Maximum buffer size to store messages (bytes): 2000
    POP3: Client: Packet time out (seconds): 1
    POP3: Client: Connection time out (seconds): 30
    POP3: Client: Disconnect time out (seconds): 2
    POP3: Client: TCP socket send wait (seconds): 2
    POP3: Client: Server reply timeout (seconds): 10
    POP3: Client: TCP window size (bytes): 1460
    POP3: Client: Maximum user name length (bytes): 40
    POP3: Client: Maximum password length (bytes): 20
    FTP: Server: Internal thread priority: 16
    FTP: Server: Internal thread time slicing interval  (ticks): 2
    FTP: Server: Maximum clients to serve simultaneously: 4
    FTP: Server: Control window size (bytes): 400
    FTP: Server: Data window size (bytes): 2048
    FTP: Server: Duration internal services will suspend for (seconds): 1
    FTP: Server: Maximum username length (bytes): 20
    FTP: Server: Maximum password length (bytes): 20
    FTP: Server: Duration allowed with no activity (seconds): 240
    FTP: Server: Socket retransmit timeout (seconds): 2
    FTP: Server: Maximum queued transmit packets: 20
    FTP: Server: Number of socket retransmissions: 10
    FTP: Server: Binary left shift as multiplier for next retry duration: 2
    HTTP: Server: FileX Support: Enable
    HTTP: Server: Multipart HTTP requests support: Disable
    HTTP: Server: Internal thread priority: 16
    HTTP: Server: Internal thread time slicing interval (ticks): 2
    HTTP: Server: Server socket window size (bytes): 2048
    HTTP: Server: Server time out (seconds): 10
    HTTP: Server: Server time out for accept (seconds): 10
    HTTP: Server: Server time out for disconnect (seconds): 10
    HTTP: Server: Server time out for receive (seconds): 10
    HTTP: Server: Server time out for send (seconds): 10
    HTTP: Server: Maximum size of header field (bytes): 256
    HTTP: Server: Maximum connections in queue: 5
    HTTP: Server: Maximum client user name length (bytes): 20
    HTTP: Server: Maximum client user password length (bytes): 20
    HTTP: Server: Minimum size of packets in pool (bytes): 600
    HTTP: Server: Maximum number of queued transmit packets (units): 20
    HTTP: Server: Wait before retry (seconds): 2
    HTTP: Server: Maximum number of retries per packet: 10
    HTTP: Server: Binary left shift as multiplier for next retry duration: 1
    TFTP: Server: FileX support: Enable
    TFTP: Server: Retransmission on client request support: Disable
    TFTP: Server: Internal thread priority: 16
    TFTP: Server: Maximum clients to serve simultaneously: 10
    TFTP: Server: Time slice for internal thread: 2
    TFTP: Server: Client request activity timeout check interval (ticks): 20
    TFTP: Server: Ack or data retransmission interval (ticks): 200
    TFTP: Server: Maximum retries for transmission without response: 5
    TFTP: Server: Maximum retries for transmission with duplicate response: 2
    Web HTTP: Server: HTTPS Support: Disable
    Web HTTP: Server: FileX Support: Enable
    Web HTTP: Server: Multipart HTTP requests support: Disable
    Web HTTP: Server: Server thread priority: 16
    Web HTTP: Server: Server thread time slicing interval (ticks): 2
    Web HTTP: Server: Server socket window size (bytes): 2048
    Web HTTP: Server: Server time out (seconds): 10
    Web HTTP: Server: Server time out for accept (seconds): 10
    Web HTTP: Server: Server time out for disconnect (seconds): 10
    Web HTTP: Server: Server time out for receive (seconds): 10
    Web HTTP: Server: Server time out for send (seconds): 10
    Web HTTP: Server: Maximum size of header field (bytes): 256
    Web HTTP: Server: Maximum connections in queue: 4
    Web HTTP: Server: Maximum length of resource name: 40
    Web HTTP: Server: Number of simultaneous sessions for server: 2
    Web HTTP: Server: Minimum size of packets in pool (bytes): 600
    Web HTTP: Server: Maximum number of queued transmit packets (units): 20
    Web HTTP: Server: Server Socket Re-transmission Timeout (seconds): 2
    Web HTTP: Server: Maximum number of retries per packet: 10
    Web HTTP: Server: Server Next Re-transmission timeout shift: 1
    Common: TCP/IP Offload: Enable
    Common: Interface Capability: Enable
    
  Module "Azure RTOS NetX Duo Packet Pool Instance"
    Common: Error Checking: Enabled (default)
    Common: IP Packet Filter: Disabled (default)
    Common: IP Static Routing: Disabled (default)
    Common: Physical Header: 
    Common: Physical Trailer: 
    Common: ARP Defend By Reply: Disabled (default)
    Common: ARP Mac Change Notification: Disabled (default)
    Common: ARP Expiration Rate: 
    Common: ARP Update Rate: 
    Common: TCP ACK Timer Rate: 
    Common: TCP Fast Timer Rate: 
    Common: TCP Transmit Timer Rate: 
    Common: TCP Keepalive Initial: 
    Common: TCP Keepalive Retry Interval: 
    Common: ARP Maximum Retries: 
    Common: ARP Maximum Queue Depth: 
    Common: ARP Auto ARP Entry: Enabled (default)
    Common: Maximum Multicast Groups: 
    Common: Maximum Listen Requests: 
    Common: TCP Keepalive: Disabled (default)
    Common: TCP Window Scaling: Disabled (default)
    Common: TCP Immediate ACK: Disabled (default)
    Common: TCP ACK Every N Packets: 
    Common: TCP Maximum Retries: 
    Common: TCP Maximum TX Queue: 
    Common: TCP Retry Shift: 
    Common: TCP Keepalive Retries: 
    Common: Driver Deferred Processing: Disabled (default)
    Common: Loopback Interface: Enabled (default)
    Common: Maximum Physical Interfaces: 
    Common: Fragmentation support: Enabled (default)
    Common: IP RX Checksum: Enabled (default)
    Common: IP TX Checksum: Enabled (default)
    Common: TCP RX Checksum: Enabled (default)
    Common: TCP TX Checksum: Enabled (default)
    Common: UDP RX Checksum: Enabled (default)
    Common: UDP TX Checksum: Enabled (default)
    Common: Reset Disconnect: Enabled (default)
    Common: RX Size Checking: Enabled (default)
    Common: ARP Info: Enabled (default)
    Common: IP Info: Enabled (default)
    Common: ICMP Info: Enabled (default)
    Common: IGMPv2: Enabled (default)
    Common: IGMP Info: Enabled (default)
    Common: Packet Info: Enabled (default)
    Common: RARP Info: Enabled (default)
    Common: TCP Info: Enabled (default)
    Common: UDP Info: Enabled (default)
    Common: Extended Notify Support: Disabled (default)
    Common: NAT: Disabled (default)
    Common: Packet Header Pad Size: 
    Common: TCP MSS Minimum: 
    Common: Source Address Check: Disabled (default)
    Common: ARP Defend Interval: 
    Common: TCP Maximum Out Of Order Packets: 
    Common: NetX Duo IPV6 Support: Disabled
    Common: Notify when the IPv6 address is changed: Disabled (default)
    Common: Allow discover maximum MTU in the path: Disabled (default)
    Common: Wait before resetting target's path MTU in destination table (seconds): 
    Common: IPv6 routing table entry limit: 
    Common: IPv6 destination table entry limit: 
    Common: Maximum time allowed to reassemble IP fragment: 
    Common: Maximum time allowed to reassemble IPv4 fragment: 
    Common: Maximum time allowed to reassemble IPv6 fragment: 
    Common: IPv6 multicast join/leave function support: Disabled (default)
    Common: Size of the prefix table for router advertisements: 
    Common: Stateless address auto-configuration support: Disabled (default)
    Common: IPv6 address pool entry limit: 
    Common: Delay before the first stale cache entry solicitation (seconds): 
    Common: Duplicate Address Detection support: Enabled (default)
    Common: Neighbor Solicitation message count before interface address marked valid: 
    Common: Retain older cache table entries till timeout option: Disabled (default)
    Common: IPv6 Neighbor Cache table entry limit.: 
    Common: Neighbor Solicitation message count for IPv6 Neighbor Discovery protocol: 
    Common: Neighbor Solicitation message count to determine neighbor’s reachability: 
    Common: Maximum entries in ND cache queue: 
    Common: Duration for address to be 'reachable' with no packets received from it (seconds): 
    Common: Delay between solicitation packets (milliseconds): 
    Common: ICMPv6 error message in response to invalid packet support: Enabled (default)
    Common: ICMPv6 redirect packet processing support: Enabled (default)
    Common: IPv6 router advertisement packet processing support: Enabled (default)
    Common: Periodic IPv6 router solicitation messages support: Enabled (default)
    Common: Maximum host router solicitations till no response is received: 
    Common: Interval between two router solicitation messages: 
    Common: Checksum computation support on received ICMPv4 packets: Enabled (default)
    Common: Checksum computation support on received ICMPv6 packets: Enabled (default)
    Common: Checksum computation support on received ICMP packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMPv4 packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMPv6 packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMP packets: Enabled (default)
    Common: Packet Alignment: 
    Common: Random Number Generator: rand
    Common: Seed Random Number Generator: srand
    DHCP: Common: IPv4: Type of Service for UDP requests: Normal
    DHCP: Common: IPv4: Fragmentation option: Don't fragment
    DHCP: Common: IPv4: Time to live: 128
    DHCP: Common: IPv4: Packet Queue depth: 5
    DHCP: Client: IPv4: Internal thread priority: 3
    DHCP: Client: IPv4: Internal thread stack size (bytes): 4096
    DHCP: Client: IPv4: Timeout between DHCP messages processed (seconds): 1
    DHCP: Client: IPv4: Use BOOTP: Disable
    DHCP: Client: IPv4: Send ARP probe: Disable
    DHCP: Client: IPv4: ARP probe wait time (seconds): 1
    DHCP: Client: IPv4: Minimum ARP probe wait time (seconds): 1
    DHCP: Client: IPv4: Maximum ARP probe wait time (seconds): 2
    DHCP: Client: IPv4: ARP probe count: 2
    DHCP: Client: IPv4: Maximum retransmission timeout (seconds): 64
    DHCP: Client: IPv4: Minimum renew timeout (seconds): 60
    DHCP: Client: IPv4: Minimum retransmission timeout (seconds): 4
    DHCP: Client: IPv4: Persistent client state: Disable
    DHCP: Client: IPv4: Maximum message size support: Disable
    DHCP: Client: IPv4: DHCP options buffer size (bytes): 312
    DHCP: Client: IPv4: Maximum number of network interfaces for DHCP client: 1
    DHCP: Client: IPv4: Wait before restarting the configuration process (seconds): 10
    HTTP: Common: Type of Service: Normal
    HTTP: Common: Fragmentation option: Don't fragment
    HTTP: Common: Time to live: 128
    HTTP: Common: MD5 Support: Disable
    HTTP: Common: Maximum resource name length (bytes): 40
    HTTP: Common: Maximum password length (bytes): 20
    HTTP: Common: Maximum username length (bytes): 20
    HTTP: Client: Minimum packet size (bytes): 600
    HTTP: Client: Operation timeout (seconds): 10
    DNS: Client: DNS Control Type of Service: Normal
    DNS: Client: Socket fragmentation option: Dont fragment
    DNS: Client: Time to live: 128
    DNS: Client: Client DNS IP version: IPv4
    DNS: Client: Maximum number of DNS Servers in the Client server list: 5
    DNS: Client: Maximum DNS queries size (bytes): 512
    DNS: Client: Maximum retries for a server: 3
    DNS: Client: Maximum duration to retransmit a DNS query (seconds): 64
    DNS: Client: Packet allocate timeout (seconds): 1
    DNS: Client: Client has DNS and Gateway server: Disable
    DNS: Client: Clear previous DNS queries from queue: Disable
    DNS: Client: Extended RR types support: Disable
    DNS: Client: Cache support: Disable
    Telnet: Common: Type of service for TCP requests: Normal
    Telnet: Common: Fragmentation option: Don't fragment
    Telnet: Common: Server TCP port number: 23
    Telnet: Common: Time to live: 128
    AutoIP: Wait before sending first probe (seconds): 1
    AutoIP: ARP probes to send: 3
    AutoIP: Minimum wait between probes (seconds): 1
    AutoIP: Maximum wait between probes (seconds): 2
    AutoIP: Maximum conflicts before increasing processing delay: 10
    AutoIP: Wait extend after maximum conflicts (seconds): 60
    AutoIP: Wait before announcement (seconds): 2
    AutoIP: Number of ARP announces: 2
    AutoIP: Wait between announces (seconds): 2
    AutoIP: Wait between defense announces (seconds): 10
    Web HTTP: Common: Type of Service: Normal
    Web HTTP: Common: Fragmentation option: Don't fragment
    Web HTTP: Common: MD5 Support: Disable
    Web HTTP: Common: Time to live: 128
    Web HTTP: Common: Maximum password length (bytes): 20
    Web HTTP: Common: Maximum username length (bytes): 20
    Web HTTP: Client: Minimum packet size (bytes): 300
    Web HTTP: Client: HTTPS Support: Disable
    SMTP: Client: TCP window size (bytes): 1460
    SMTP: Client: Packet allocation timeout (seconds): 2
    SMTP: Client: TCP socket connect timeout (seconds): 10
    SMTP: Client: TCP socket disconnect timeout (seconds): 5
    SMTP: Client: Server greeting reply timeout (seconds): 10
    SMTP: Client: Command timeout (seconds): 10
    SMTP: Client: Mail data request timeout (seconds): 30
    SMTP: Client: TCP socket send completion timeout (seconds): 5
    SMTP: Client: Server challenge maximum string length (bytes): 200
    SMTP: Client: Maximum password length (bytes): 20
    SMTP: Client: Maximum username length (bytes): 40
    DHCP: Client: IPv6: Internal thread priority: 3
    DHCP: Client: IPv6: Time out for obtaining DHCPv6 client mutex (ticks): TX_WAIT_FOREVER
    DHCP: Client: IPv6: Time interval between current IP address lease time update (seconds): 1
    DHCP: Client: IPv6: Maximum IA addresses allowed in client record: 1
    DHCP: Client: IPv6: Number of DNS servers the client will store: 2
    DHCP: Client: IPv6: Number of time servers the client will store: 1
    DHCP: Client: IPv6: Domain name buffer size (bytes): 32
    DHCP: Client: IPv6: Current time zone information buffer size (bytes): 16
    DHCP: Client: IPv6: Maximum DHCPv6 server messages buffer size (bytes): 100
    DHCP: Common: IPv6: Type of Service for UDP requests: Normal
    DHCP: Common: IPv6: Time to live: 128
    DHCP: Common: IPv6: Packet Queue depth: 5
    DHCP: Common: IPv6: Packet allocation timeout (seconds): 3
    DHCP: Common: IPv6: Interval for active session time update (seconds): 3
    DHCP: Server: IPv4: Internal thread priority: 2
    DHCP: Server: IPv4: Packet allocate timeout (seconds): 2
    DHCP: Server: IPv4: Fast periodic timer interval to check session inactivity timeout (seconds): 10
    DHCP: Server: IPv4: DHCP Client Session timeout - multiple of Fast periodic interval (seconds): 10
    DHCP: Server: IPv4: Client IP address default lease time (seconds): 0xFFFFFFFF
    DHCP: Server: IPv4: Slow periodic timer interval to check IP lease expiration (seconds): 1000
    DHCP: Server: IPv4: Size of the array to contain options in client request (units): 12
    DHCP: Server: IPv4: Server option list (optional - use space for separation) : 1 3 6
    DHCP: Server: IPv4: Server option list size (optional): 3
    DHCP: Server: IPv4: Size of the server host name buffer (bytes): 32
    DHCP: Server: IPv4: Size of the current client hostname buffer (bytes): 32
    DHCP: Server: IPv4: Maximum size of an IP addresses list (units): 20
    DHCP: Server: IPv4: Size of client record table (units): 50
    DHCP: Server: IPv4: Size of the BOOT buffer (bytes): 548
    DHCP: Server: IPv6: Internal thread priority: 2
    DHCP: Server: IPv6: Client lease time expiration check interval (seconds): 60
    DHCP: Server: IPv6: DHCPv6 packet receive timeout (seconds): 1
    DHCP: Server: IPv6: Server preference ranking for clients: 0
    DHCP: Server: IPv6: Maximum options to extract from a client message: 6
    DHCP: Server: IPv6: Server interval for first client IP address renewal attempt (seconds): 2000
    DHCP: Server: IPv6: Server interval for second client IP address renewal attempt (seconds): 3000
    DHCP: Server: IPv6: Time interval after which client IP is deprecated (seconds): 2 * NX_DHCPV6_DEFAULT_T1_TIME
    DHCP: Server: IPv6: Time interval after which leased IP is invalid (seconds): 2 * NX_DHCPV6_DEFAULT_PREFERRED_TIME
    DHCP: Server: IPv6: Maximum server status option message size (bytes): 100
    DHCP: Server: IPv6: Maximum Size of the Server’s IP lease table (count): 100
    DHCP: Server: IPv6: Size of the Server’s Client record table (count): 120
    DHCP: Server: IPv6: Server socket fragmentation option: Dont fragment
    DHCP: Server: IPv6: Vendor assigned unique ID: abcdeffghijklmnopqrstuvwxyz
    DHCP: Server: IPv6: Private vendor ID: 0x12345678
    DHCP: Server: IPv6: Size of Vendor ID buffer (bytes): 48
    DHCP: Server: IPv6: Client request success message : granted: IA OPTION GRANTED
    DHCP: Server: IPv6: Client request failure message : Failure unspecified: IA OPTION NOT GRANTED-FAILURE UNSPECIFIED
    DHCP: Server: IPv6: Client request failure message : No addresses available: IA OPTION NOT GRANTED-NO ADDRESSES AVAILABLE
    DHCP: Server: IPv6: Client request failure message : Invalid client request: IA OPTION NOT GRANTED-INVALID CLIENT REQUEST
    DHCP: Server: IPv6: Client request failure message : Client not on link: IA OPTION NOT GRANTED-CLIENT NOT ON LINK
    DHCP: Server: IPv6: Client request failure message : Client must use multicast: IA OPTION NOT GRANTED-CLIENT MUST USE MULTICAST
    DHCP: Server: IPv6: Session inactivity timeout(seconds): 20
    Telnet: Server: Internal thread priority: 16
    Telnet: Server: Maximum clients to serve simultaneously: 4
    Telnet: Server: Socket window size (bytes): 2048
    Telnet: Server: Server time out (seconds): 10
    Telnet: Server: Client inactivity timeout (seconds): 600
    Telnet: Server: Timeout check period (seconds): 60
    Telnet: Server: Option negotiation: Enable
    Telnet: Server: Use application packet pool: Disable
    Telnet: Server: Packet size in the pool (bytes): 300
    Telnet: Server: Total packet pool size (bytes): 2048
    SNTP: Client: Internal thread stack size (bytes): 2048
    SNTP: Client: SNTP client thread time slicing interval (ticks): TX_NO_TIME_SLICE
    SNTP: Client: Internal thread priority: 2
    SNTP: Client: UDP socket name: SNTP Client socket
    SNTP: Client: UDP port number: 123
    SNTP: Client: Server UDP port: 123
    SNTP: Client: Time to live: 128
    SNTP: Client: Maximum UDP packets queue depth (units): 5
    SNTP: Client: Packet allocation timeout (seconds): 1
    SNTP: Client: SNTP version to use: 3
    SNTP: Client: NTP minimum version: 3
    SNTP: Client: Lowest level server stratum client accepts: 2
    SNTP: Client: Minimum time difference that triggers adjustment (milliseconds): 10
    SNTP: Client: Maximum time adjustment allowed to local clock time (milliseconds): 180000
    SNTP: Client: Ignore maximum time adjust limit at startup: True
    SNTP: Client: Maximum time lapse without valid update (seconds): 7200
    SNTP: Client: 'Update time remaining' timer update interval (seconds): 1
    SNTP: Client: Starting poll interval for unicast update request (seconds): 3600
    SNTP: Client: Poll interval increment after failed time update: 2
    SNTP: Client: Calculate round trip time of messages: False
    SNTP: Client: Maximum server clock inaccuracy to accept (to disable set 0): 50000
    SNTP: Client: Invalid message limit to mark server invalid: 3
    SNTP: Client: Randomize update request interval on startup: False
    SNTP: Client: Internal Task sleep interval (ticks): 1
    SNTP: Client: Current calendar year: 2016
    TFTP: Common: Maximum error string length (bytes): 64
    TFTP: Common: Time to live: 128
    TFTP: Common: Type of Service for UDP requests: Normal
    TFTP: Common: Fragmentation option: Don't fragment
    TFTP: Client: Source port to use: NX_ANY_PORT
    MQTT: Client: NX Secure: Disable
    MQTT: Client: Cloud Enable: Disable
    MQTT: Client: Keepalive Timer Rate (s): 1
    MQTT: Client: Ping Timeout Delay (s): 1
    MQTT: Client: Socket Timeout (in timer ticks) : 0xFFFFFFFF
    NAT: Minimum count for translation entry: 3
    NAT: Timeout for translation entry (seconds): 240
    NAT: Minimum assigned port number for outbound TCP packets: 20000
    NAT: Maximum assigned port number for outbound TCP packets: 30000
    NAT: Minimum assigned port number for outbound UDP packets: 20000
    NAT: Maximum assigned port number for outbound UDP packets: 30000
    NAT: Minimum ICMP query identifier: 20000
    NAT: Maximum ICMP query identifier: 30000
    FTP: Common: Control Type of Service: Normal
    FTP: Common: Data Type of Service: Normal
    FTP: Common: Fragmentation option: Don't fragment
    FTP: Common: Time to live: 128
    FTP: Common: Duration between client inactivity check (seconds): 60
    FTP: Client: TCP socket to use: NX_ANY_PORT
    SNMP: Agent: Internal thread stack size (bytes): 4096
    SNMP: Agent: SNMP agent priority: 16
    SNMP: Agent: Type of service for SNMP responses: Normal
    SNMP: Agent: Fragment enable for SNMP PDU requests: Dont Fragment
    SNMP: Agent: SNMP socket time to live: 128
    SNMP: Agent: Agent timeout: 100
    SNMP: Agent: Max octet string size: 255
    SNMP: Agent: Max context string size: 32
    SNMP: Agent: Max User name Size: 64
    SNMP: Agent: Max security Key Size: 64
    SNMP: Agent: Maximum SNMP packet size: 560
    SNMP: Agent: UDP port number: 161
    SNMP: Agent: Trap destination port: 162
    SNMP: Agent: Max trap Key Size: 64
    SNMP: Agent: SNMP Version 1: Enable
    SNMP: Agent: SNMP Version 2: Enable
    SNMP: Agent: SNMP Version 3: Enable
    POP3: Client: Maximum buffer size to store messages (bytes): 2000
    POP3: Client: Packet time out (seconds): 1
    POP3: Client: Connection time out (seconds): 30
    POP3: Client: Disconnect time out (seconds): 2
    POP3: Client: TCP socket send wait (seconds): 2
    POP3: Client: Server reply timeout (seconds): 10
    POP3: Client: TCP window size (bytes): 1460
    POP3: Client: Maximum user name length (bytes): 40
    POP3: Client: Maximum password length (bytes): 20
    FTP: Server: Internal thread priority: 16
    FTP: Server: Internal thread time slicing interval  (ticks): 2
    FTP: Server: Maximum clients to serve simultaneously: 4
    FTP: Server: Control window size (bytes): 400
    FTP: Server: Data window size (bytes): 2048
    FTP: Server: Duration internal services will suspend for (seconds): 1
    FTP: Server: Maximum username length (bytes): 20
    FTP: Server: Maximum password length (bytes): 20
    FTP: Server: Duration allowed with no activity (seconds): 240
    FTP: Server: Socket retransmit timeout (seconds): 2
    FTP: Server: Maximum queued transmit packets: 20
    FTP: Server: Number of socket retransmissions: 10
    FTP: Server: Binary left shift as multiplier for next retry duration: 2
    HTTP: Server: FileX Support: Enable
    HTTP: Server: Multipart HTTP requests support: Disable
    HTTP: Server: Internal thread priority: 16
    HTTP: Server: Internal thread time slicing interval (ticks): 2
    HTTP: Server: Server socket window size (bytes): 2048
    HTTP: Server: Server time out (seconds): 10
    HTTP: Server: Server time out for accept (seconds): 10
    HTTP: Server: Server time out for disconnect (seconds): 10
    HTTP: Server: Server time out for receive (seconds): 10
    HTTP: Server: Server time out for send (seconds): 10
    HTTP: Server: Maximum size of header field (bytes): 256
    HTTP: Server: Maximum connections in queue: 5
    HTTP: Server: Maximum client user name length (bytes): 20
    HTTP: Server: Maximum client user password length (bytes): 20
    HTTP: Server: Minimum size of packets in pool (bytes): 600
    HTTP: Server: Maximum number of queued transmit packets (units): 20
    HTTP: Server: Wait before retry (seconds): 2
    HTTP: Server: Maximum number of retries per packet: 10
    HTTP: Server: Binary left shift as multiplier for next retry duration: 1
    TFTP: Server: FileX support: Enable
    TFTP: Server: Retransmission on client request support: Disable
    TFTP: Server: Internal thread priority: 16
    TFTP: Server: Maximum clients to serve simultaneously: 10
    TFTP: Server: Time slice for internal thread: 2
    TFTP: Server: Client request activity timeout check interval (ticks): 20
    TFTP: Server: Ack or data retransmission interval (ticks): 200
    TFTP: Server: Maximum retries for transmission without response: 5
    TFTP: Server: Maximum retries for transmission with duplicate response: 2
    Web HTTP: Server: HTTPS Support: Disable
    Web HTTP: Server: FileX Support: Enable
    Web HTTP: Server: Multipart HTTP requests support: Disable
    Web HTTP: Server: Server thread priority: 16
    Web HTTP: Server: Server thread time slicing interval (ticks): 2
    Web HTTP: Server: Server socket window size (bytes): 2048
    Web HTTP: Server: Server time out (seconds): 10
    Web HTTP: Server: Server time out for accept (seconds): 10
    Web HTTP: Server: Server time out for disconnect (seconds): 10
    Web HTTP: Server: Server time out for receive (seconds): 10
    Web HTTP: Server: Server time out for send (seconds): 10
    Web HTTP: Server: Maximum size of header field (bytes): 256
    Web HTTP: Server: Maximum connections in queue: 4
    Web HTTP: Server: Maximum length of resource name: 40
    Web HTTP: Server: Number of simultaneous sessions for server: 2
    Web HTTP: Server: Minimum size of packets in pool (bytes): 600
    Web HTTP: Server: Maximum number of queued transmit packets (units): 20
    Web HTTP: Server: Server Socket Re-transmission Timeout (seconds): 2
    Web HTTP: Server: Maximum number of retries per packet: 10
    Web HTTP: Server: Server Next Re-transmission timeout shift: 1
    Common: TCP/IP Offload: Enable
    Common: Interface Capability: Enable
    
  Module "NetX Duo WiFi Driver (rm_netxduo_wifi)"
    IP MTU (bytes): 1500
    
  Module "WiFi Onchip Silex Driver using r_sci_uart (rm_wifi_onchip_silex)"
    Parameter Checking: Default (BSP)
    Number of supported socket instances: 1
    Size of TX buffer for CMD Port: 1500
    Size of RX buffer for CMD Port: 3000
    Semaphore maximum timeout: 10000
    Number of retries for AT commands: 10
    Module Reset Port: 04
    Module Reset Pin: 03
    Enable SNTP Client: Disabled
    Max SSID Length: 32
    Max BSSID Length: 6
    Max Passphrase Length: 32
    
  Module "UART (r_sci_uart)"
    Parameter Checking: Default (BSP)
    FIFO Support: Enable
    DTC Support: Enable
    Flow Control Support: Disable
    RS-485 Support: Disable
    
  Module "Azure RTOS NetX Duo Common"
    Common: Error Checking: Enabled (default)
    Common: IP Packet Filter: Disabled (default)
    Common: IP Static Routing: Disabled (default)
    Common: Physical Header: 
    Common: Physical Trailer: 
    Common: ARP Defend By Reply: Disabled (default)
    Common: ARP Mac Change Notification: Disabled (default)
    Common: ARP Expiration Rate: 
    Common: ARP Update Rate: 
    Common: TCP ACK Timer Rate: 
    Common: TCP Fast Timer Rate: 
    Common: TCP Transmit Timer Rate: 
    Common: TCP Keepalive Initial: 
    Common: TCP Keepalive Retry Interval: 
    Common: ARP Maximum Retries: 
    Common: ARP Maximum Queue Depth: 
    Common: ARP Auto ARP Entry: Enabled (default)
    Common: Maximum Multicast Groups: 
    Common: Maximum Listen Requests: 
    Common: TCP Keepalive: Disabled (default)
    Common: TCP Window Scaling: Disabled (default)
    Common: TCP Immediate ACK: Disabled (default)
    Common: TCP ACK Every N Packets: 
    Common: TCP Maximum Retries: 
    Common: TCP Maximum TX Queue: 
    Common: TCP Retry Shift: 
    Common: TCP Keepalive Retries: 
    Common: Driver Deferred Processing: Disabled (default)
    Common: Loopback Interface: Enabled (default)
    Common: Maximum Physical Interfaces: 
    Common: Fragmentation support: Enabled (default)
    Common: IP RX Checksum: Enabled (default)
    Common: IP TX Checksum: Enabled (default)
    Common: TCP RX Checksum: Enabled (default)
    Common: TCP TX Checksum: Enabled (default)
    Common: UDP RX Checksum: Enabled (default)
    Common: UDP TX Checksum: Enabled (default)
    Common: Reset Disconnect: Enabled (default)
    Common: RX Size Checking: Enabled (default)
    Common: ARP Info: Enabled (default)
    Common: IP Info: Enabled (default)
    Common: ICMP Info: Enabled (default)
    Common: IGMPv2: Enabled (default)
    Common: IGMP Info: Enabled (default)
    Common: Packet Info: Enabled (default)
    Common: RARP Info: Enabled (default)
    Common: TCP Info: Enabled (default)
    Common: UDP Info: Enabled (default)
    Common: Extended Notify Support: Disabled (default)
    Common: NAT: Disabled (default)
    Common: Packet Header Pad Size: 
    Common: TCP MSS Minimum: 
    Common: Source Address Check: Disabled (default)
    Common: ARP Defend Interval: 
    Common: TCP Maximum Out Of Order Packets: 
    Common: NetX Duo IPV6 Support: Disabled
    Common: Notify when the IPv6 address is changed: Disabled (default)
    Common: Allow discover maximum MTU in the path: Disabled (default)
    Common: Wait before resetting target's path MTU in destination table (seconds): 
    Common: IPv6 routing table entry limit: 
    Common: IPv6 destination table entry limit: 
    Common: Maximum time allowed to reassemble IP fragment: 
    Common: Maximum time allowed to reassemble IPv4 fragment: 
    Common: Maximum time allowed to reassemble IPv6 fragment: 
    Common: IPv6 multicast join/leave function support: Disabled (default)
    Common: Size of the prefix table for router advertisements: 
    Common: Stateless address auto-configuration support: Disabled (default)
    Common: IPv6 address pool entry limit: 
    Common: Delay before the first stale cache entry solicitation (seconds): 
    Common: Duplicate Address Detection support: Enabled (default)
    Common: Neighbor Solicitation message count before interface address marked valid: 
    Common: Retain older cache table entries till timeout option: Disabled (default)
    Common: IPv6 Neighbor Cache table entry limit.: 
    Common: Neighbor Solicitation message count for IPv6 Neighbor Discovery protocol: 
    Common: Neighbor Solicitation message count to determine neighbor’s reachability: 
    Common: Maximum entries in ND cache queue: 
    Common: Duration for address to be 'reachable' with no packets received from it (seconds): 
    Common: Delay between solicitation packets (milliseconds): 
    Common: ICMPv6 error message in response to invalid packet support: Enabled (default)
    Common: ICMPv6 redirect packet processing support: Enabled (default)
    Common: IPv6 router advertisement packet processing support: Enabled (default)
    Common: Periodic IPv6 router solicitation messages support: Enabled (default)
    Common: Maximum host router solicitations till no response is received: 
    Common: Interval between two router solicitation messages: 
    Common: Checksum computation support on received ICMPv4 packets: Enabled (default)
    Common: Checksum computation support on received ICMPv6 packets: Enabled (default)
    Common: Checksum computation support on received ICMP packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMPv4 packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMPv6 packets: Enabled (default)
    Common: Checksum computation support on transmitted ICMP packets: Enabled (default)
    Common: Packet Alignment: 
    Common: Random Number Generator: rand
    Common: Seed Random Number Generator: srand
    DHCP: Common: IPv4: Type of Service for UDP requests: Normal
    DHCP: Common: IPv4: Fragmentation option: Don't fragment
    DHCP: Common: IPv4: Time to live: 128
    DHCP: Common: IPv4: Packet Queue depth: 5
    DHCP: Client: IPv4: Internal thread priority: 3
    DHCP: Client: IPv4: Internal thread stack size (bytes): 4096
    DHCP: Client: IPv4: Timeout between DHCP messages processed (seconds): 1
    DHCP: Client: IPv4: Use BOOTP: Disable
    DHCP: Client: IPv4: Send ARP probe: Disable
    DHCP: Client: IPv4: ARP probe wait time (seconds): 1
    DHCP: Client: IPv4: Minimum ARP probe wait time (seconds): 1
    DHCP: Client: IPv4: Maximum ARP probe wait time (seconds): 2
    DHCP: Client: IPv4: ARP probe count: 2
    DHCP: Client: IPv4: Maximum retransmission timeout (seconds): 64
    DHCP: Client: IPv4: Minimum renew timeout (seconds): 60
    DHCP: Client: IPv4: Minimum retransmission timeout (seconds): 4
    DHCP: Client: IPv4: Persistent client state: Disable
    DHCP: Client: IPv4: Maximum message size support: Disable
    DHCP: Client: IPv4: DHCP options buffer size (bytes): 312
    DHCP: Client: IPv4: Maximum number of network interfaces for DHCP client: 1
    DHCP: Client: IPv4: Wait before restarting the configuration process (seconds): 10
    HTTP: Common: Type of Service: Normal
    HTTP: Common: Fragmentation option: Don't fragment
    HTTP: Common: Time to live: 128
    HTTP: Common: MD5 Support: Disable
    HTTP: Common: Maximum resource name length (bytes): 40
    HTTP: Common: Maximum password length (bytes): 20
    HTTP: Common: Maximum username length (bytes): 20
    HTTP: Client: Minimum packet size (bytes): 600
    HTTP: Client: Operation timeout (seconds): 10
    DNS: Client: DNS Control Type of Service: Normal
    DNS: Client: Socket fragmentation option: Dont fragment
    DNS: Client: Time to live: 128
    DNS: Client: Client DNS IP version: IPv4
    DNS: Client: Maximum number of DNS Servers in the Client server list: 5
    DNS: Client: Maximum DNS queries size (bytes): 512
    DNS: Client: Maximum retries for a server: 3
    DNS: Client: Maximum duration to retransmit a DNS query (seconds): 64
    DNS: Client: Packet allocate timeout (seconds): 1
    DNS: Client: Client has DNS and Gateway server: Disable
    DNS: Client: Clear previous DNS queries from queue: Disable
    DNS: Client: Extended RR types support: Disable
    DNS: Client: Cache support: Disable
    Telnet: Common: Type of service for TCP requests: Normal
    Telnet: Common: Fragmentation option: Don't fragment
    Telnet: Common: Server TCP port number: 23
    Telnet: Common: Time to live: 128
    AutoIP: Wait before sending first probe (seconds): 1
    AutoIP: ARP probes to send: 3
    AutoIP: Minimum wait between probes (seconds): 1
    AutoIP: Maximum wait between probes (seconds): 2
    AutoIP: Maximum conflicts before increasing processing delay: 10
    AutoIP: Wait extend after maximum conflicts (seconds): 60
    AutoIP: Wait before announcement (seconds): 2
    AutoIP: Number of ARP announces: 2
    AutoIP: Wait between announces (seconds): 2
    AutoIP: Wait between defense announces (seconds): 10
    Web HTTP: Common: Type of Service: Normal
    Web HTTP: Common: Fragmentation option: Don't fragment
    Web HTTP: Common: MD5 Support: Disable
    Web HTTP: Common: Time to live: 128
    Web HTTP: Common: Maximum password length (bytes): 20
    Web HTTP: Common: Maximum username length (bytes): 20
    Web HTTP: Client: Minimum packet size (bytes): 300
    Web HTTP: Client: HTTPS Support: Disable
    SMTP: Client: TCP window size (bytes): 1460
    SMTP: Client: Packet allocation timeout (seconds): 2
    SMTP: Client: TCP socket connect timeout (seconds): 10
    SMTP: Client: TCP socket disconnect timeout (seconds): 5
    SMTP: Client: Server greeting reply timeout (seconds): 10
    SMTP: Client: Command timeout (seconds): 10
    SMTP: Client: Mail data request timeout (seconds): 30
    SMTP: Client: TCP socket send completion timeout (seconds): 5
    SMTP: Client: Server challenge maximum string length (bytes): 200
    SMTP: Client: Maximum password length (bytes): 20
    SMTP: Client: Maximum username length (bytes): 40
    DHCP: Client: IPv6: Internal thread priority: 3
    DHCP: Client: IPv6: Time out for obtaining DHCPv6 client mutex (ticks): TX_WAIT_FOREVER
    DHCP: Client: IPv6: Time interval between current IP address lease time update (seconds): 1
    DHCP: Client: IPv6: Maximum IA addresses allowed in client record: 1
    DHCP: Client: IPv6: Number of DNS servers the client will store: 2
    DHCP: Client: IPv6: Number of time servers the client will store: 1
    DHCP: Client: IPv6: Domain name buffer size (bytes): 32
    DHCP: Client: IPv6: Current time zone information buffer size (bytes): 16
    DHCP: Client: IPv6: Maximum DHCPv6 server messages buffer size (bytes): 100
    DHCP: Common: IPv6: Type of Service for UDP requests: Normal
    DHCP: Common: IPv6: Time to live: 128
    DHCP: Common: IPv6: Packet Queue depth: 5
    DHCP: Common: IPv6: Packet allocation timeout (seconds): 3
    DHCP: Common: IPv6: Interval for active session time update (seconds): 3
    DHCP: Server: IPv4: Internal thread priority: 2
    DHCP: Server: IPv4: Packet allocate timeout (seconds): 2
    DHCP: Server: IPv4: Fast periodic timer interval to check session inactivity timeout (seconds): 10
    DHCP: Server: IPv4: DHCP Client Session timeout - multiple of Fast periodic interval (seconds): 10
    DHCP: Server: IPv4: Client IP address default lease time (seconds): 0xFFFFFFFF
    DHCP: Server: IPv4: Slow periodic timer interval to check IP lease expiration (seconds): 1000
    DHCP: Server: IPv4: Size of the array to contain options in client request (units): 12
    DHCP: Server: IPv4: Server option list (optional - use space for separation) : 1 3 6
    DHCP: Server: IPv4: Server option list size (optional): 3
    DHCP: Server: IPv4: Size of the server host name buffer (bytes): 32
    DHCP: Server: IPv4: Size of the current client hostname buffer (bytes): 32
    DHCP: Server: IPv4: Maximum size of an IP addresses list (units): 20
    DHCP: Server: IPv4: Size of client record table (units): 50
    DHCP: Server: IPv4: Size of the BOOT buffer (bytes): 548
    DHCP: Server: IPv6: Internal thread priority: 2
    DHCP: Server: IPv6: Client lease time expiration check interval (seconds): 60
    DHCP: Server: IPv6: DHCPv6 packet receive timeout (seconds): 1
    DHCP: Server: IPv6: Server preference ranking for clients: 0
    DHCP: Server: IPv6: Maximum options to extract from a client message: 6
    DHCP: Server: IPv6: Server interval for first client IP address renewal attempt (seconds): 2000
    DHCP: Server: IPv6: Server interval for second client IP address renewal attempt (seconds): 3000
    DHCP: Server: IPv6: Time interval after which client IP is deprecated (seconds): 2 * NX_DHCPV6_DEFAULT_T1_TIME
    DHCP: Server: IPv6: Time interval after which leased IP is invalid (seconds): 2 * NX_DHCPV6_DEFAULT_PREFERRED_TIME
    DHCP: Server: IPv6: Maximum server status option message size (bytes): 100
    DHCP: Server: IPv6: Maximum Size of the Server’s IP lease table (count): 100
    DHCP: Server: IPv6: Size of the Server’s Client record table (count): 120
    DHCP: Server: IPv6: Server socket fragmentation option: Dont fragment
    DHCP: Server: IPv6: Vendor assigned unique ID: abcdeffghijklmnopqrstuvwxyz
    DHCP: Server: IPv6: Private vendor ID: 0x12345678
    DHCP: Server: IPv6: Size of Vendor ID buffer (bytes): 48
    DHCP: Server: IPv6: Client request success message : granted: IA OPTION GRANTED
    DHCP: Server: IPv6: Client request failure message : Failure unspecified: IA OPTION NOT GRANTED-FAILURE UNSPECIFIED
    DHCP: Server: IPv6: Client request failure message : No addresses available: IA OPTION NOT GRANTED-NO ADDRESSES AVAILABLE
    DHCP: Server: IPv6: Client request failure message : Invalid client request: IA OPTION NOT GRANTED-INVALID CLIENT REQUEST
    DHCP: Server: IPv6: Client request failure message : Client not on link: IA OPTION NOT GRANTED-CLIENT NOT ON LINK
    DHCP: Server: IPv6: Client request failure message : Client must use multicast: IA OPTION NOT GRANTED-CLIENT MUST USE MULTICAST
    DHCP: Server: IPv6: Session inactivity timeout(seconds): 20
    Telnet: Server: Internal thread priority: 16
    Telnet: Server: Maximum clients to serve simultaneously: 4
    Telnet: Server: Socket window size (bytes): 2048
    Telnet: Server: Server time out (seconds): 10
    Telnet: Server: Client inactivity timeout (seconds): 600
    Telnet: Server: Timeout check period (seconds): 60
    Telnet: Server: Option negotiation: Enable
    Telnet: Server: Use application packet pool: Disable
    Telnet: Server: Packet size in the pool (bytes): 300
    Telnet: Server: Total packet pool size (bytes): 2048
    SNTP: Client: Internal thread stack size (bytes): 2048
    SNTP: Client: SNTP client thread time slicing interval (ticks): TX_NO_TIME_SLICE
    SNTP: Client: Internal thread priority: 2
    SNTP: Client: UDP socket name: SNTP Client socket
    SNTP: Client: UDP port number: 123
    SNTP: Client: Server UDP port: 123
    SNTP: Client: Time to live: 128
    SNTP: Client: Maximum UDP packets queue depth (units): 5
    SNTP: Client: Packet allocation timeout (seconds): 1
    SNTP: Client: SNTP version to use: 3
    SNTP: Client: NTP minimum version: 3
    SNTP: Client: Lowest level server stratum client accepts: 2
    SNTP: Client: Minimum time difference that triggers adjustment (milliseconds): 10
    SNTP: Client: Maximum time adjustment allowed to local clock time (milliseconds): 180000
    SNTP: Client: Ignore maximum time adjust limit at startup: True
    SNTP: Client: Maximum time lapse without valid update (seconds): 7200
    SNTP: Client: 'Update time remaining' timer update interval (seconds): 1
    SNTP: Client: Starting poll interval for unicast update request (seconds): 3600
    SNTP: Client: Poll interval increment after failed time update: 2
    SNTP: Client: Calculate round trip time of messages: False
    SNTP: Client: Maximum server clock inaccuracy to accept (to disable set 0): 50000
    SNTP: Client: Invalid message limit to mark server invalid: 3
    SNTP: Client: Randomize update request interval on startup: False
    SNTP: Client: Internal Task sleep interval (ticks): 1
    SNTP: Client: Current calendar year: 2016
    TFTP: Common: Maximum error string length (bytes): 64
    TFTP: Common: Time to live: 128
    TFTP: Common: Type of Service for UDP requests: Normal
    TFTP: Common: Fragmentation option: Don't fragment
    TFTP: Client: Source port to use: NX_ANY_PORT
    MQTT: Client: NX Secure: Disable
    MQTT: Client: Cloud Enable: Disable
    MQTT: Client: Keepalive Timer Rate (s): 1
    MQTT: Client: Ping Timeout Delay (s): 1
    MQTT: Client: Socket Timeout (in timer ticks) : 0xFFFFFFFF
    NAT: Minimum count for translation entry: 3
    NAT: Timeout for translation entry (seconds): 240
    NAT: Minimum assigned port number for outbound TCP packets: 20000
    NAT: Maximum assigned port number for outbound TCP packets: 30000
    NAT: Minimum assigned port number for outbound UDP packets: 20000
    NAT: Maximum assigned port number for outbound UDP packets: 30000
    NAT: Minimum ICMP query identifier: 20000
    NAT: Maximum ICMP query identifier: 30000
    FTP: Common: Control Type of Service: Normal
    FTP: Common: Data Type of Service: Normal
    FTP: Common: Fragmentation option: Don't fragment
    FTP: Common: Time to live: 128
    FTP: Common: Duration between client inactivity check (seconds): 60
    FTP: Client: TCP socket to use: NX_ANY_PORT
    SNMP: Agent: Internal thread stack size (bytes): 4096
    SNMP: Agent: SNMP agent priority: 16
    SNMP: Agent: Type of service for SNMP responses: Normal
    SNMP: Agent: Fragment enable for SNMP PDU requests: Dont Fragment
    SNMP: Agent: SNMP socket time to live: 128
    SNMP: Agent: Agent timeout: 100
    SNMP: Agent: Max octet string size: 255
    SNMP: Agent: Max context string size: 32
    SNMP: Agent: Max User name Size: 64
    SNMP: Agent: Max security Key Size: 64
    SNMP: Agent: Maximum SNMP packet size: 560
    SNMP: Agent: UDP port number: 161
    SNMP: Agent: Trap destination port: 162
    SNMP: Agent: Max trap Key Size: 64
    SNMP: Agent: SNMP Version 1: Enable
    SNMP: Agent: SNMP Version 2: Enable
    SNMP: Agent: SNMP Version 3: Enable
    POP3: Client: Maximum buffer size to store messages (bytes): 2000
    POP3: Client: Packet time out (seconds): 1
    POP3: Client: Connection time out (seconds): 30
    POP3: Client: Disconnect time out (seconds): 2
    POP3: Client: TCP socket send wait (seconds): 2
    POP3: Client: Server reply timeout (seconds): 10
    POP3: Client: TCP window size (bytes): 1460
    POP3: Client: Maximum user name length (bytes): 40
    POP3: Client: Maximum password length (bytes): 20
    FTP: Server: Internal thread priority: 16
    FTP: Server: Internal thread time slicing interval  (ticks): 2
    FTP: Server: Maximum clients to serve simultaneously: 4
    FTP: Server: Control window size (bytes): 400
    FTP: Server: Data window size (bytes): 2048
    FTP: Server: Duration internal services will suspend for (seconds): 1
    FTP: Server: Maximum username length (bytes): 20
    FTP: Server: Maximum password length (bytes): 20
    FTP: Server: Duration allowed with no activity (seconds): 240
    FTP: Server: Socket retransmit timeout (seconds): 2
    FTP: Server: Maximum queued transmit packets: 20
    FTP: Server: Number of socket retransmissions: 10
    FTP: Server: Binary left shift as multiplier for next retry duration: 2
    HTTP: Server: FileX Support: Enable
    HTTP: Server: Multipart HTTP requests support: Disable
    HTTP: Server: Internal thread priority: 16
    HTTP: Server: Internal thread time slicing interval (ticks): 2
    HTTP: Server: Server socket window size (bytes): 2048
    HTTP: Server: Server time out (seconds): 10
    HTTP: Server: Server time out for accept (seconds): 10
    HTTP: Server: Server time out for disconnect (seconds): 10
    HTTP: Server: Server time out for receive (seconds): 10
    HTTP: Server: Server time out for send (seconds): 10
    HTTP: Server: Maximum size of header field (bytes): 256
    HTTP: Server: Maximum connections in queue: 5
    HTTP: Server: Maximum client user name length (bytes): 20
    HTTP: Server: Maximum client user password length (bytes): 20
    HTTP: Server: Minimum size of packets in pool (bytes): 600
    HTTP: Server: Maximum number of queued transmit packets (units): 20
    HTTP: Server: Wait before retry (seconds): 2
    HTTP: Server: Maximum number of retries per packet: 10
    HTTP: Server: Binary left shift as multiplier for next retry duration: 1
    TFTP: Server: FileX support: Enable
    TFTP: Server: Retransmission on client request support: Disable
    TFTP: Server: Internal thread priority: 16
    TFTP: Server: Maximum clients to serve simultaneously: 10
    TFTP: Server: Time slice for internal thread: 2
    TFTP: Server: Client request activity timeout check interval (ticks): 20
    TFTP: Server: Ack or data retransmission interval (ticks): 200
    TFTP: Server: Maximum retries for transmission without response: 5
    TFTP: Server: Maximum retries for transmission with duplicate response: 2
    Web HTTP: Server: HTTPS Support: Disable
    Web HTTP: Server: FileX Support: Enable
    Web HTTP: Server: Multipart HTTP requests support: Disable
    Web HTTP: Server: Server thread priority: 16
    Web HTTP: Server: Server thread time slicing interval (ticks): 2
    Web HTTP: Server: Server socket window size (bytes): 2048
    Web HTTP: Server: Server time out (seconds): 10
    Web HTTP: Server: Server time out for accept (seconds): 10
    Web HTTP: Server: Server time out for disconnect (seconds): 10
    Web HTTP: Server: Server time out for receive (seconds): 10
    Web HTTP: Server: Server time out for send (seconds): 10
    Web HTTP: Server: Maximum size of header field (bytes): 256
    Web HTTP: Server: Maximum connections in queue: 4
    Web HTTP: Server: Maximum length of resource name: 40
    Web HTTP: Server: Number of simultaneous sessions for server: 2
    Web HTTP: Server: Minimum size of packets in pool (bytes): 600
    Web HTTP: Server: Maximum number of queued transmit packets (units): 20
    Web HTTP: Server: Server Socket Re-transmission Timeout (seconds): 2
    Web HTTP: Server: Maximum number of retries per packet: 10
    Web HTTP: Server: Server Next Re-transmission timeout shift: 1
    Common: TCP/IP Offload: Enable
    Common: Interface Capability: Enable
    
  Azure RTOS ThreadX
    General: Custom tx_user.h: 
    General: Error Checking: Enabled
    Timer: Timer Ticks Per Second: 100
    General: Max Priorities: 32
    General: Minimum Stack: 200
    Timer: Timer Thread Stack Size: 1024
    Timer: Timer Thread Priority: 01
    Timer: Timer Process In ISR: Enabled
    Timer: Reactivate Inline: Disabled
    General: Stack Filling: Enabled
    General: Preemption Threshold: Disabled
    Timer: Timer: Enabled
    General: Notify Callbacks: Disabled
    General: Inline Thread Resume Suspend: Disabled
    General: Not Interruptable: Disabled
    Trace: Event Trace: Disabled
    Trace: Trace Buffer Name: g_tx_trace_buffer
    Trace: Memory section for Trace Buffer: .bss
    Trace: Trace Buffer Size: 65536
    Trace: Trace Buffer Number of Registries: 30
    Performance: Block Pool Performance Info: Disabled
    Performance: Byte Pool Performance Info: Disabled
    Performance: Event Flags Performance Info: Disabled
    Performance: Mutex Performance Info: Disabled
    Performance: Queue Performance Info: Disabled
    Performance: Semaphore Performance Info: Disabled
    Performance: Thread Performance Info: Disabled
    Performance: Timer Performance Info: Disabled
    RA: Hardware Thread Stack Monitoring: Disabled
    Interrupts: SysTick Interrupt Priority: Priority 0 (highest)
    Interrupts: Maximum Interrupt Priority: Priority 0 (highest)
    General: IAR Library Support: Disabled
    General: BSD Support: Disabled
    General: FileX Pointer: Enabled
    
  HAL
    Instance "g_ioport I/O Port (r_ioport)"
      Name: g_ioport
      Port 1 ELC Trigger Source: Disabled
      Port 2 ELC Trigger Source: Disabled
      Port 3 ELC Trigger Source: Disabled
      Port 4 ELC Trigger Source: Disabled
      Port B ELC Trigger Source: Disabled
      Port C ELC Trigger Source: Disabled
      Port D ELC Trigger Source: Disabled
      Port E ELC Trigger Source: Disabled
      Pin Configuration Name: g_bsp_pin_cfg
      
    Instance "Azure RTOS ThreadX Port (rm_threadx_port)"
  Thread "Azure Wifi Thread"
    Symbol: azure_wifi_thread
    Name: Azure Wifi Thread
    Stack size (bytes): 4096
    Priority: 4
    Auto start: Enabled
    Time slicing interval (ticks): 1
    
    Instance "g_ip0 Azure RTOS NetX Duo IP Instance"
      Name: g_ip0
      IPv4 Address: 192.168.0.2
      Subnet Mask: 0.0.0.0
      Default Gateway Address: 192.168.0.1
      IPv6 Global Address: 2001:0:0:0:0:0:0:1
      IPv6 Link Local Address (All zeros means use MAC address): 0:0:0:0:0:0:0:0
      IP Helper Thread Stack Size (bytes): 2048
      IP Helper Thread Priority: 3
      ARP cache storage units: Bytes
          ARP cache size (in storage units): 520
      
      Instance "g_packet_pool0 Azure RTOS NetX Duo Packet Pool Instance"
        Name: g_packet_pool0
        Packet Size (bytes): 1568
        Number of Packets in Pool: 16
        
      Instance "NetX Duo WiFi Driver (rm_netxduo_wifi)"
        AP SSID: 
        AP Password: 
        AP Security: WPA2
        
        Instance "WiFi Onchip Silex Driver using r_sci_uart (rm_wifi_onchip_silex)"
          SNTP server IPv4 address: 0.0.0.0
          STNP Timezone Offset from UTC Hours: 0
          STNP Timezone Offset from UTC Minutes: 0
          Use Daylight Savings Time: Disabled
          
          Instance "g_uart0 UART (r_sci_uart)"
            General: Name: g_uart0
            General: Channel: 4
            General: Data Bits: 8bits
            General: Parity: None
            General: Stop Bits: 1bit
            Baud: Baud Rate: 115200
            Baud: Baud Rate Modulation: Disabled
            Baud: Max Error (%): 5
            Flow Control: CTS/RTS Selection: Hardware RTS
            Flow Control: Software RTS Port: Disabled
            Flow Control: Software RTS Pin: Disabled
            Extra: Clock Source: Internal Clock
            Extra: Start bit detection: Falling Edge
            Extra: Noise Filter: Disable
            Extra: Receive FIFO Trigger Level: Max
            Extra: RS-485: DE Pin: Disable
            Extra: RS-485: DE Pin Polarity: Active High
            Extra: RS-485: DE Port Number: Disabled
            Extra: RS-485: DE Pin Number: Disabled
            Interrupts: Callback: rm_wifi_onchip_silex_uart_callback
            Interrupts: Receive Interrupt Priority: Priority 12
            Interrupts: Transmit Data Empty Interrupt Priority: Priority 12
            Interrupts: Transmit End Interrupt Priority: Priority 12
            Interrupts: Error Interrupt Priority: Priority 12
            
        Instance "Azure RTOS NetX Duo Common"
  Thread "RTT Thread"
    Symbol: rtt_thread
    Name: RTT Thread
    Stack size (bytes): 8192
    Priority: 5
    Auto start: Enabled
    Time slicing interval (ticks): 1
    
