/***********************************************************************************************************************
* Copyright [2020] Renesas Electronics Corporation and/or its affiliates.  All Rights Reserved.
*
* This software is supplied by Renesas Electronics America Inc. and may only be used with products of Renesas Electronics Corp.
* and its affiliates (“Renesas”).  No other uses are authorized.  This software is protected under all applicable laws, 
* including copyright laws.
* Renesas reserves the right to change or discontinue this software.
* THE SOFTWARE IS DELIVERED TO YOU “AS IS,” AND RENESAS MAKES NO REPRESENTATIONS OR WARRANTIES, AND TO THE FULLEST EXTENT 
* PERMISSIBLE UNDER APPLICABLE LAW,DISCLAIMS ALL WARRANTIES, WHETHER EXPLICITLY OR IMPLICITLY, INCLUDING WARRANTIES OF 
* MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, AND NONINFRINGEMENT, WITH RESPECT TO THE SOFTWARE.  TO THE MAXIMUM 
* EXTENT PERMITTED BY LAW, IN NO EVENT WILL RENESAS BE LIABLE TO YOU IN CONNECTION WITH THE SOFTWARE (OR ANY PERSON 
* OR ENTITY CLAIMING RIGHTS DERIVED FROM YOU) FOR ANY LOSS, DAMAGES, OR CLAIMS WHATSOEVER, INCLUDING, WITHOUT LIMITATION, 
* ANY DIRECT, CONSEQUENTIAL, SPECIAL, INDIRECT, PUNITIVE, OR INCIDENTAL DAMAGES;
* ANY LOST PROFITS, OTHER ECONOMIC DAMAGE, PROPERTY DAMAGE, OR PERSONAL INJURY; AND EVEN IF RENESAS HAS BEEN ADVISED OF 
* THE POSSIBILITY OF SUCH LOSS,DAMAGES, CLAIMS OR COSTS.
* **********************************************************************************************************************/

Project Overview:
	The example projects demonstrates Message Queue and Semaphore between tasks and interrupt. Message Queue is demonstrated 
	between Tasks and between Task and interrupt. GPT timer periodically generates interrupt at 1000msec. For first few seconds, 
	messages are shared between Sender and Receiver Tasks and GPT0 ISR. Receiver task pends on Message Queue, receives and 
	displays message received on RTT viewer periodically at 500msec. For next few seconds, Semaphore Task waits for sempahore 
	until it is released by GPT1 ISR. GPT1 ISR releases semaphore periodically at 1000msec. All the tasks run with equal 
	priority level.
   
﻿
1) Segger RTT block address may be needed to download and observe EP operation using a hex file with RTT-Viewer.
   RTT Block address for hex file committed in repository are as follows:
   a. e2studio: 0x20000054
   b. Keil:	0x20000010
   c. IAR: 0x200018e8
 
2) If an EP is modified, compiled, and downloaded please find the block address (for the variable in RAM called _SEGGER_RTT) 
   in .map file generated in the build configuration folder (Debug/Release).
