"--endian=little" 

"--cpu=Cortex-M33" 

"--cmse" 

"--drv_vector_table_base=0x0" 

"--fpu=VFPv5_SP" 

"-p" 

"c:\Program Files\IAR Systems\Embedded Workbench 9.0\arm\CONFIG\debugger\Renesas\R7FA4M2AD.ddf" 

"--semihosting" 

"--device=R7FA4M2AD" 

"--drv_communication=USB0" 

"--drv_interface_speed=auto" 

"--jlink_initial_speed=1000" 

"--jlink_reset_strategy=0,0" 

"--drv_interface=SWD" 

"--drv_catch_exceptions=0x000" 

"--drv_swo_clock_setup=50000000,0,2000000" 




