/***********************************************************************************************************************
* Copyright [2020] Renesas Electronics Corporation and/or its affiliates.  All Rights Reserved.
*
* This software is supplied by Renesas Electronics America Inc. and may only be used with products of Renesas Electronics Corp.
* and its affiliates (“Renesas”).  No other uses are authorized.  This software is protected under all applicable laws, 
* including copyright laws.
* Renesas reserves the right to change or discontinue this software.
* THE SOFTWARE IS DELIVERED TO YOU “AS IS,” AND RENESAS MAKES NO REPRESENTATIONS OR WARRANTIES, AND TO THE FULLEST EXTENT 
* PERMISSIBLE UNDER APPLICABLE LAW,DISCLAIMS ALL WARRANTIES, WHETHER EXPLICITLY OR IMPLICITLY, INCLUDING WARRANTIES OF 
* MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, AND NONINFRINGEMENT, WITH RESPECT TO THE SOFTWARE.  TO THE MAXIMUM 
* EXTENT PERMITTED BY LAW, IN NO EVENT WILL RENESAS BE LIABLE TO YOU IN CONNECTION WITH THE SOFTWARE (OR ANY PERSON 
* OR ENTITY CLAIMING RIGHTS DERIVED FROM YOU) FOR ANY LOSS, DAMAGES, OR CLAIMS WHATSOEVER, INCLUDING, WITHOUT LIMITATION, 
* ANY DIRECT, CONSEQUENTIAL, SPECIAL, INDIRECT, PUNITIVE, OR INCIDENTAL DAMAGES;
* ANY LOST PROFITS, OTHER ECONOMIC DAMAGE, PROPERTY DAMAGE, OR PERSONAL INJURY; AND EVEN IF RENESAS HAS BEEN ADVISED OF 
* THE POSSIBILITY OF SUCH LOSS,DAMAGES, CLAIMS OR COSTS.
* **********************************************************************************************************************/

1. Project Overview:
	This Example Project demonstrates the functionality of AGT in periodic mode and one-shot mode.  On providing any 
input on the RTTviewer, AGT channel 0 starts in one-shot mode. AGT channel 1 starts in periodic mode when AGT channel 0 expires.
Timer in periodic mode expires periodically at a time period specified by user and toggles the on-board LED.
	
NOTE:
1. User is expected to enter data of size not exceeding above 15 bytes.
   Operation is not guaranteed for any user input value other than integer,char(i.e. float, special char) through RTT.


	





 
﻿
1) Segger RTT block address may be needed to download and observe EP operation using a hex file with RTT-Viewer.
   RTT Block address for hex file committed in repository are as follows:
   a. e2studio: 0x200000ac
   b. Keil:	0x2000000c
   c. IAR: 0x2000023c
 
2) If an EP is modified, compiled, and downloaded please find the block address (for the variable in RAM called _SEGGER_RTT) 
   in .map file generated in the build configuration folder (Debug/Release).
